    Super Sound Canvas Roland SC-88

    The SC-88 Sound Canvas is a professional quality General MIDI sound
    module designed for an extensive range of music applications.

    The SC-88's increased channels, voices, sounds, signal processing and
    improved sound quality make it the perfect choice for demanding
    applications.

    Power that transcends conventional sound modules.

    The SC-88 is in a class by itself. With 32-part multitimbral
    capability and 64-note polyphony, there are two independant MIDI
    inputs for utilizing the SC-88's awesome multitimbral capability.

    To take advantage of all 32 channels, you can use the Roland MC-50MkII
    Microcomposer, or a PC-based sequencing system equipped with Roland's
    Super-MPU MIDI Interface to create intricate music with just a single
    SC-88. Until now, you could only get this much performance using
    multiple sound modules, but one SC-88 can function as two complete
    Roland SC-55MkII sound modules.

    Sound - incredible quality matched by quantity.

    The SC-88 utilizes 18-bit D/A conversion for breathtaking sound
    quality with true CD S/N ratio and wide dynamic range. All appropriate
    instruments have been meticulously multisampled to provide a more
    expressive and natural sound over the entire pitch range.

    The SC-88's 8 Mbyte wave memory is equivalent to 16 Mbytes in a 16-bit
    linear format, allowing the SC-88 to offer an immense number of sounds
    that include General MIDI System Level 1 and the Roland GS Format
    sounds. You can create full-scale orchestration ensembles by selecting
    from 654 different instruments.

    These built-in sounds include 300 outstanding sounds carefully
    selected from the highly rated Roland JV-80/880 synthesizers and
    SR-JV80 Series expansion boards as well as S-Series Sampler CD-ROM
    sounds. Particularly noteworthy are the numerous acoustic instrument
    types, including piano, guitar, strings and brass. Twenty-two drum
    sets and two SFX sets are also included. There is also a separate
    SC-55 Map button on the front panel if SC-55MkII sounds are desired.

    For each of the SC-88's 32 Parts, you can select any sound desired -
    from realistic acoustic instruments to the latest and various synth
    textures - for use in virtually any kind of musical genre.

    Powerful onboard digital effects.

    The SC-88 incorporates professional signal processing capabilities
    with digital reverb, digital chorus, digital delay and 2-band EQ. Each
    Part can store its own effects send leveland on/off status as well as
    EQ on/off settings.

    The high-quality and versatility of these effects are perfect for
    slight processing or radical sound creation.

    Sound editing that delivers professional results.

    Editing capabilities on the SC-88 are comparable to those found on
    advanced synthesizers, yet are even more convenient to use. The front
    panel edit button allows quick access to vibrato, filter and envelope
    parameter values for easily altering instrument sounds.

    The SC-88 stores 256 User Instruments and two User Drum Sets. You can
    also edit each Part using detuning, octave, modulation and portamento.
    Any Part of MIDI In B can be layered with the sound in the same Part
    of MIDI In A for more creative sound options.

    Enhanced operational use.

    The SC-88's front panel features a large, graphic display that remains
    easily readable, even while displaying a considerable amount of
    information such as bar-graph levels for 16 Parts. Operational
    settings are remarkably easy to adjust with the SC-88's front panel
    buttons. Even advanced functions can easily be adjusted with a minimal
    number of buttons.

    Additional features ensure total versatility.

    The SC-88 is equipped with MIDI In A/B connectors on the rear panel as
    well as a front panel MIDI In B. This extra MIDI connector can be
    conveniently used with an external MIDI controller like the Roland
    AX-1 and A-30 for realtime performances.

    The built-in serial port on the SC-88's rear panel allows you to
    directly connect an IBM/compatible or Macintosh computer via RS-232C
    or RS-422 interface ports without using a MIDI interface.

    The Stereo Audio In jack has an input volume control knob for
    efficient mixing without the need of an external audio mixer.

    A convenient Preview button lets you instantly hear the internal sound
    assigned to a Part.

    The Solo button allows you to isolate a specific part while song data
    is being played back. The All monitor function alows all Parts to be
    monitored even if multiple Parts are muted. The Part information
    function displays voice, bender, modulation, expression, portamento,
    hold, soft and sostenuto information received by any specific part.

    All SC-88 settings, other than default settings, can be transmitted to
    a connected sequencer. This allows MIDI bulk dumps to contain a
    smaller volume of data. By recording these settings at the beginning
    of a song you can ensure accurate playback of your song files.

    Useful peripherals extend the SC-88's operational scope.

    For utilizing the maximum potential of the SC-88, Roland provides
    various peripherals capable of controlling its 32 Parts.

    MC-50MkII Micro Composer
    A MIDI sequencer with two individual MIDI outputs that support 32 MIDI
    channels.

    S-MPU/AT Super MPU MIDI Interface
    An intelligent MIDI interface for IBM/compatible computers with two
    individual MIDI outputs that support 32 MIDI Channels

    654 incredible sounds stored in the 8 Mbyte internal memory -
    equivalent to 16 Mbytes in 16-bit linear format.

    64-voice polyphony easily accomodates full orchestrations and lush
    instrumentation.

    32-Part multitimbrality with two individual MIDI inputs allows you to
    create and play back complex sequences with a new level of freedom and
    flexibility.

    24 drum sets including two SFX sets to facilitate music composition in
    any genre and style.

    18-bit D/A conversion ensures true CD-quality sound with the purity
    and transparency associated with expensive high-end sound modules.

    Specifications (subject to change without notice)

    - Number of Parts
      32 (using MIDI In A and B simultaneously)
    - Maximum Polyphony
      64
    - Sound Generation
      PCM based sound source with TVF
    - Wave Memory
      8 Mbytes (equivalent to 16 Mbytes in a 16-bit linear format), 654
      Inst. + 22 Drum Sets + 2 SFX sets
    - User Memory
      256 User Inst. + 2 User Drum Sets
    - Built-in Effects
      Reverb, Chorus, Delay, EQ
    - Display
      Custom LCD (70.6mm x 24.5mm) with backlighting
    - Connectors & Jacks
      MIDI In A, In B (front,rear), Out/Thru
      Audio Input (L, R) (with Input Volume Control),
      Audio Output (L, R), Computer, Headphones
    - Dimensions
      218 (W) x 250 (D) x 72 (H) mm
      (8-5/8" x 9-7/8" x 2-7/8")
    - Weight
      2.6 Kg (5 lbs 12 oz)
    - Options
      RAD-50 Rackmount Adaptor

    Effects Types and Parameters
              +----------------------------------+-----------------------------+
              |Type                              | Parameter                   |
    +---------+----------------------------------+-----------------------------+
    |Reverb   |Room 1,2,3,4, Hall 1,2, Plate,    | Character, Pre LPF, Level,  |
    |         |Delay, Panning Delay              | Time, Delay feedback, Pre   |
    |         |                                  | Delay Time, Part Send Level |
    +---------+----------------------------------+-----------------------------+
    |Chorus   |Chorus 1,2,3,4, Feedback Chorus,  | Pre LPF, Level, Feedback,   |
    |         |Flanger, Short Delay, Short Delay | Delay, Rate, Depth, Send    |
    |         |(FB)                              | Level to Reverb, Send level |
    |         |                                  | to Delay, Part Send Level   |
    +---------+----------------------------------+-----------------------------+
    |Delay    |Delay 1,2,3,4, Pan Delay 1,2,3,4, | Pre LPF, Delay Time Center, |
    |         |Delay to Reverb, Pan Repeat       | Delay Time Ratio L/R, Level |
    |         |                                  | Center/L/R, Level, Feedback,|
    |         |                                  | Send Level to Reverb, Part  |
    |         |                                  | Send Level                  |
    +---------+----------------------------------+-----------------------------+
    |Equalizer|                                  | Low Freq. (100/200Hz), High |
    |         |                                  | Freq. (4k/8kHz), Low Gain   |
    |         |                                  | (+-12dB), High Gain (+-     |
    |         |                                  | 12dB), Part EQ (On/Off)     |
    +---------+----------------------------------+-----------------------------+

    SC-88 Preset Instruments and Drum Sets(*)
    +----------------------+-----------------+-----------+-------------+
    | Group                | SC-55MkII Inst. | New Inst. # SC-88 Total |
    +----------------------+-----------------+-----------+-------------+
    | Piano                |   21            |   25      #   46        |
    +----------------------+-----------------+-----------+-------------+
    | Chromatic Percussion |   12            |   12      #   24        |
    +----------------------+-----------------+-----------+-------------+
    | Organ                |   16            |   28      #   44        |
    +----------------------+-----------------+-----------+-------------+
    | Guitar               |   19            |   31      #   50        |
    +----------------------+-----------------+-----------+-------------+
    | Bass                 |   12            |   29      #   41        |
    +----------------------+-----------------+-----------+-------------+
    | Strings/Orchestra    |    9            |   11      #   20        |
    +----------------------+-----------------+-----------+-------------+
    | Ensemble             |   11            |   24      #   35        |
    +----------------------+-----------------+-----------+-------------+
    | Brass                |   15            |   21      #   36        |
    +----------------------+-----------------+-----------+-------------+
    | Reed                 |    8            |   11      #   19        |
    +----------------------+-----------------+-----------+-------------+
    | Pipe                 |    8            |    5      #   13        |
    +----------------------+-----------------+-----------+-------------+
    | Synth Lead           |   12            |   19      #   31        |
    +----------------------+-----------------+-----------+-------------+
    | Synth Pad            |    8            |   12      #   20        |
    +----------------------+-----------------+-----------+-------------+
    | Synth SFX            |   11            |   31      #   42        |
    +----------------------+-----------------+-----------+-------------+
    | Ethnic               |   10            |   16      #   26        |
    +----------------------+-----------------+-----------+-------------+
    | Percussive           |   13            |   17      #   30        |
    +----------------------+-----------------+-----------+-------------+
    | SFX                  |   41            |    8      #   49        |
    +----------------------+-----------------+-----------+-------------+
    | CM-64 compatible     |  128            |    -      #  128        |
    +======================+=================+===========+=============+
    | Preset Inst. Total   |  354            |  300      #  654        |
    +----------------------+-----------------+-----------+-------------+

    +------------------------+------------------+
    |   SC-55MkII Drum Set   |   New Drum Set   |
    +------------------------+------------------+
    |   Standard             |   Standard 1     |
    +------------------------+------------------+
    |   Room                 |   Standard 2     |
    +------------------------+------------------+
    |   Power                |   Room           |
    +------------------------+------------------+
    |   Electronic           |   Power          |
    +------------------------+------------------+
    |   TR-808               |   Electronic     |
    +------------------------+------------------+
    |   Jazz                 |   TR-808/909     |
    +------------------------+------------------+
    |   Brush                |   Dance          |
    +------------------------+------------------+
    |   Orchestra            |   Jazz           |
    +------------------------+------------------+
    |   SFX                  |   Brush          |
    +------------------------+------------------+
    |   CM-64                |   Orchestra      |
    +------------------------+------------------+
    |                        |   Ethnic         |
    +------------------------+------------------+
    |                        |   Kick & Snare   |
    +------------------------+------------------+
    |                        |   SFX            |
    +------------------------+------------------+
    |                        |   Rythm FX       |
    +========================+==================+
    |  9 + SFX               |   13 + SFX       |
    +------------------------+------------------+

    (*) Similarly named configurations of the SC-55MkII and New drum sets differ.

    { Typographical errors are mine. Semantic errors are Roland's. :) }