================================
RE:   82C928 MAD16 Release 2.05
================================

To: 	OPTi Customer
Date:	07/19/94
==================================================================

0) What's New in this version

   This version has been enhanced from 2.04. Changes added are:
   1.) Fix for Hard Disk Hang up on one in-house machine.

   2.) Fix for bug found in update of AUTOEXEC.BAT file. Older versions
       did not add newline before "REM** OPTi ..." statement during
       installation.

   3.) Support for DOS Games in Windows:
       Current implementation is designed for those DOS games which have
       icons in Windows and run in full screen DOS and close after finished. 
       When multiple DOS boxes are open, only the first DOS box owns the 
       audio device. DOS Box support could be very complicated, in relative 
       very short period of development time we have to concentrate our 
       implementation only on those features most useful to the general users. 
       We recommend to run game or play audio in DOS box only one at a time. 
       Close the DOS box which owns the device will return the device to 
       Windows. Then you can play audio in Windows or run another DOS game.

       !! Note !!
       Sometimes, the Setup of the PIF file of a DOS game is crucial. 
       To make a game work effectively under Windows, you probably have 
       to try a few alternative options through PIF editor.
      

1) Introduction

   This package contains the above version of Software release for 
   OPTi 82C928 Audio Device. This software contains a basic installer 
   for 82C928 DOS and Windows drivers.

2) File List of the 928v205e.ZIP

   For the general release diskette,

     INSTALL.EXE	;  the installation program
     INSTALL.001	;  the compressed installation files
     INSTALL.DAT	;  installation script file
     			;  customers may change this to customize for 
			;  themselves
     README.TXT		;  latest release information;
     			;  customers MUST change this file themselves to
			;  reflect their latest product info.
     DISK.ID		;  the disk ID for installation purpose

   For OPTi customers in-house use,
       
     README.1st		; this document

3) How to create an Install Diskette from 928v205e.ZIP

   . unZIP the 928v205e.ZIP file into a temp. dir in hard Drive
   . take out README.1st 
   . copy all the files in this temp. dir into an empty floppy
   . use this floppy as an INSTALL diskette

   To Run the INSTALLER
   
   . insert the INSTALL diskette into a: or b: drive
   . type a:\INSTALL or b:\INSTALL


