Latest Updates to the Manuals                Multimedia Pro Sound Card Ver 2.0
-----------------------------                ---------------------------------

This file contains information about changes made after the manual has been 
printed.

The contents are as follows:

A.  Installing the utilities and software
B.  SGPFIG.EXE program
C.  INSTATCD.EXE program

A.  Installing the utilities and software
-----------------------------------------

The installation program for the utilities and software is now expanded to 
do the following:

- copy all the appropriate files from the floppy diskettes into your PC's 
  harddisk.

- configure the I/O Base Address, Interrupt Setting, DMA Channel Setting 
  for the sound card.

- check that there is no conflict for the configuration that you have chosen.

- setup all Windows software in the Windows environment.

- install all Windows drivers in the Windows environment.

To run the install program,

1.  Insert the Multimedia Pro Sound Card Disk #1 into your A: or B: drive.

2.  Go to your A: or B: drive, and type in the following command to start 
    the install program:

    INSTALL  [Enter]
    
3.  Follow the instructions on the screen.

Note! This install program eliminates the need for you to setup any of 
      the Windows bundled software that comes with this package, i.e., WinDAT, 
      Jukebox, Monologue for Windows, and the Mixer Utility for Windows.
      
      This install program also eliminates the need for you to manually 
      install the Windows drivers.
      
    
B.  SGPFIG.EXE program
----------------------

The "AT-Bus CD-ROM Setting" option in the SGPFIG.EXE configuration program is
changed to include a Sony CD-ROM drive option. 

OLD                             NEW
---                             ---
Panasonic                       Panasonic
Mitsumi                         Mitsumi/Sony                               

If you are connecting a Sony CDU-31A CD-ROM drive, you have to select the
"Mitsumi/Sony" setting for this option when you are running this configuration
program.

Note! To connect a Sony CDU-31A CD-ROM drive to this Sound Card, you can 
      purchase the Sound Galaxy Sony Adaptor accessory from your nearest 
      Multimedia Pro Sound Card dealer.


C.  INSTATCD.EXE program
------------------------    

The INSTATCD.EXE program to install the AT-Bus CD-ROM drivers has been upgraded
to be more user-friendly.  The new program now works as follows:

Note! You must have a copy of the file MSCDEX.EXE stored in the relevant 
      location on your PC's harddisk.  It is recommended that you copy this 
      file to the \MMPRO\DRIVERS directory before running this program 
      (SGNXPRO is the default directory name, and will be different if you
      have specified a different name during installation).
       
1.  Run the program by typing INSTATCD at the \MMPRO directory, and then 
    press the [Enter] key.

    The first screen displays the three different types of AT-Bus CD-ROM 
    drivers (Panasonic, Mitsumi and Sony) to install.

2.  Select the appropriate choice.

    The program will search for the file MSCDEX.EXE on the current drive.
    If it is not found, you will be prompted for the drive where MSCDEX.EXE 
    is located.
    
If you are installing the Mitsumi CD-ROM drivers, step #3 will be displayed.
If you are installing the Panasonic or Sony CD-ROM drivers, go to step #4.

3.  For Mitsumi CD-ROM drivers, you must specify an interrupt channel for the 
    CD-ROM drive.  Select the interrupt channel (the default, IRQ 11, will 
    usually work, unless it is already used for another device). 

4.  The program will prompt you to automatically update the AUTOEXEC.BAT and 
    CONFIG.SYS files. Type [Y] to add the appropriate information into both 
    files, and exit this installation program.
    
                        
                               - end of file -
