SAM Driver for Baum SuperVario and Humanware (Pulsedata) Brailliant Braille Displays.

This is a fully functional SAM driver for use with SuperVario and Brailliant refreshable Braille displays.

This driver will support all current models.

Please report any bugs to Dolphin. If it crashes please tell us the crash address and registers etc, from the crash message box, also report the driver version number (check with explorer - file properties).

Features
Auto-detects Braille displays.
Version for Win32 (desktop version of SAM) and PDA (Pocket SAM) are available.
Supports serial connection. The PDA version also supports bluetooth. USB connection is currently not supported but is planned for the future.

Button Layout:
B1   [ ... braille cells ... ]   B4
B2   [ ... braille cells ... ]   B5
B3   [ ... braille cells ... ]   B6

Key assignments
The following lists the default keys to press for each Braille operation.
Your screen reader may not support some of these operations.

Move to top left of window: B1+B2
Move to bottom left of window: B2+B3
Move to focus: B6
Left edge of window: B1+B4
Right edge of window: B3+B6
Move one line up: B1
Move one line down: B3
Move left one Braille display width: B2
Move right one Braille display width: B5
Move left half a Braille display width: B4+B5
Move right half a Braille display width: B5+B6
Cycle Attributes: B2+B5


[End of file]