SAM Driver for Tieman MultiBraille

This driver is for use with the Tieman MultiBraille. This includes the 45 and 85 cell models.

The MultiBraille must be set to serial communications in order to use this driver. 

This driver does not automatically detect the multibraille.
To use it first make sure your Multibraille is plugged in and switched on. Next,
enter the configuration panel, set the COM port where it is plugged in and the
type of display (40 or 80 cell), then hit OK.

Refer to your screen reader for the default key assignments.
