SAM Driver for KTS Brailloterm 32

This is a fully functional SAM driver for use with a KTS Brailloterm 32.

This driver uses the WIN32 Comms API to talk to the Braille display so will work in Windows 95 and NT, there is no 16-bit code.

To use this driver the Brailloterm 32 must be set to the Windows configuration and be using the serial port. Please refer to the manual for further details.

Please report any bugs to Dolphin. If it crashes please tell us the crash address and registers etc, from the crash message box, also report the driver version number (check with explorer - file properties).

Features
Supports multiple units simultaneously.

Key assignments
The following lists the default keys to press for each Braille operation.
Your screen reader may not support some of these operations.

Move to top left of window: key N1
Move to bottom left of window: key N3
Move to focus: key N2
Left edge of window: key N8
Right edge of window: key N9
MOve one line up: key N4
MOve one line down: key N5
Read backwards: key N6
Read forwards: key N7
Switch to Attribute mode 1: key N10
Switch to Attribute mode 2: key N11
Switch to report mode: key T2
Toggle physical layout mode: key T1
Make cursor route single click: key T3
Make cursor route double click: key T4
Make cursor route right click: key T5

1/98