Contents

A. List of Files           
B. Supported synthesizers            
C. Installation            

A. List of Files

The following files should be in a KEYNOTE directory on this disk.

*   KEYNOTE.DLL     The Accent PC driver to be used with the Keynote GOLD 
                    speech synthesizer with GOLDDEV.SYS Accent emulation.
*   READ.ME         This help file.

There is a subdirectory GOLDDEV that contains the current version of
GOLDDEV.SYS. The Accent PC emulator. Note: GOLDDEV.SYS in no longer 
needed with the new drivers. It is included on this disk for your 
convenience. It must be loaded as a device driver in your CONFIG.SYS
file (DEVICE=C:\GOLDDEV.SYS).

B. Supported synthesizers

This SSIL driver, KEYNOTE.DLL, supports all older, single language
models of the Keynote Gold synthesizer. These include the Keynote 
Gold PC, a version forthe IBM PC ISA bus; the Keynote GOLD SA, a 
stand alone battery powered portable synthesizer. 

Note: we do not recommend that you use this driver with the Keynote 
GOLD VoiceCard, a PCMCIA (PC Card) synthesizer for portable computers 
and laptops equipped with PCMCIA card slots. You should use the driver
found in the KEYNOTEI (Keynote Gold International) directory.

You may order any Keynote GOLD synthesizer with a variety of
international languages built in. The languages currently available
are English, French, Spanish, German, Italian, and Dutch. This SSIL
driver supports all multilingual Keynote Gold synthesizers.


C. Installation

To use this SSIL driver, follow the instructions that came with your
application. If the application asks you for the name of the access
device driver, select KEYNOTE. If you need to browse the driver disk
for the driver file, then look in the KEYNOTE subdirectory for the
file KEYNOTE.DLL.


