Notes On Using JFW With The Kurzweil Reading Edge

Copy the files kre.dll and kre.ini to your JFW directory.

Copy the file ssil.ini to your Windows directory.  (Note  that this
ssil.ini is specific to the KRE.)  If you have the KRE connected to a
comm port other than Comm1, change the Port line in the [SSIL] section
of ssil.ini to the comm port you are using.

in the [options] section of the file \jfw\jfw.ini,
change the Driver= line to read
	Driver=kre

Press the KRE Select Input key (bottom right of the keypad) until you
hear it say "Receive from Screen Reader"

Now run JFW.

If you do not hear the JFW intro screen, check the following items and
then try running JFW again.

Is the KRE set up to communicate at 9600 baud, 8 data-bits, 1
stop-bit, no parity.  You can check/set this using the KRE
"Communications Keypad" mode.

Check to make sure that you only have one ssil.ini file, that this
file is for the KRE, and that this file is in your Windows directory.
If you have another ssil.ini file in a directory which appears on the
DOS search path prior to the Windows directory, this file will be used instead.

Note that the KRE does not allow you to use JFW to change either the
volume or rate of speech.  You need to adjust these using the knobs on
the machine itself.
