This is your JFW authorization disk.

PLEASE NOTE:  Normally, the authorization tokens on this disk are
not meant to be installed manually.  The install scripts will prompt
you to insert this disk as a part of a normal sequence of install
operations.

If you do need to install authorization manually, read on.

Please note that the examples given use A: as the floppy, and C: as
the hard drive.  You should always substitute the proper drive
letters to match your specific system.


*** JFW 3.0 95 Only

To modify and inspect authorization for the JFW 3.0 95 only product,
the commands to use are EVMOVE and CHECK.

To install an authorization token from the A: floppy drive to the C:
hard drive, use the following command line:

A:\EVMOVE A: C:

To uninstall an authorization token from the C: hard drive to the A:
floppy drive, use the following command line:

A:\EVMOVE C: A:

To check authorizations on the floppy or hard drive, invoke CHECK
with arguments of a drive letter. For instance, to check the
authorization parameters of the disk in the A: drive, type

A:\CHECK A:




*** JFW 3.0 NT/95

To modify and inspect authorization for the JFW 3.0 NT/95 product,
the command to use is HJAUTH.

To install an authorization token from the A: floppy drive to the C:
hard drive, use the following command line:

A:\HJAUTH A: C:

To uninstall an authorization token from the C: hard drive to the A:
floppy drive, use the following command line:

A:\HJAUTH C: A:

To check authorizations on the floppy or hard drive, invoke HJAUTH
with arguments of CHECK and a drive letter. For instance, to check
the authorization parameters of the disk in the A: drive, type

A:\HJAUTH CHECK A:


If you are still having problems manually installing authorization
for JFW, please contact the Henter-Joyce technical support
department.
