TextToSpeechOpenWaveOutFile

The TextToSpeechOpenWaveOutFile call causes the specified wave file to be opened and the text-to-speech system to enter into wave-file mode. This mode indicates that the speech samples are to be written in wave format into the wave file each time TextToSpeechSpeak is called. The text-to-speech system remains in the wave-file mode until TextToSpeechCloseWaveOutFile is called

Syntax | MMRESULT TextToSpeechOpenWaveOutFile | (LPTTS_HANDLE_T phTTS, LPSTR pszFileName, DWORD dwFormat)

Parameters | LPTTS_HANDLE_T phTTS | Specifies a text-to-speech handle.
| LPSTR pszFileName | Specifies a pointer to a file name.
| DWORD dwFormat | Determines the audio sample format. It can be one of the following constants that are defined in include files mmsystem.h and ttsapi.h:

Constant | Description
WAVE_FORMAT_1M08 | Mono 8-bit, 11.025 kHz sample rate
WAVE_FORMAT_1M16 | Mono 16-bit, 11.025 kHz sample rate
WAVE_FORMAT_08M08 | Mono 8-bit, -law 8 kHz sample rate

Return Value | This call returns a value of type MMRESULT. The return value is zero if the call is successful. The return value is one of the following constants:

Constant | Description
MMSYSERR_NOERROR | Normal successful completion (zero).
MMSYSERR_INVALPARAM | An invalid parameter or an illegal wave output format was passed.
MMSYSERR_NOMEM | Memory allocation error.
MMSYSERR_ALLOCATED | A wave file is already open.
MMSYSERR_ERROR | Unable to open the wave file or unable to write to the wave file.
MMSYSERR_INVALHANDLE | The text-to-speech handle was invalid.

Comments | This call automatically resumes audio output if the text-to-speech system is in a paused state by a previously issued TextToSpeechPause call. The startup function must be called to start the text-to-speech system before calling TextToSpeechOpenWaveOutFile.
See Also | TextToSpeechCloseWaveOutFile TextToSpeechPause TextToSpeechReset TextToSpeechSpeak TextToSpeechStartup (UNIX) TextToSpeechStartup (Windows) TextToSpeechStartupEx Wave-File Mode