Window Procedure Example

static UINT uiID_Error_Message = 0;

static UNIT uiID_Buffer_Message = 0;

static UNIT uiID_Index_Message = 0;

// Window Procedure

VOID MyWndProc(LONG lParam1, LONG lParam2, DWORD dwCallbackParameter, UINT uiMsg)

{

if (uiMsg == uiID_Error_Message)

{

// lParam1 contains error code

// lParam2 contains value of MMRESULT

}

else if (uiMsg == uiID_Index_Message)

{

// lParam2 contains index mark

}

else if (uiMsg == uiID_Buffer_Message)

{

// lParam2 contains Pointer to buffer

}

}

VOID main()

{

LPTTS_HANDLE_TAG phTTS;

TextToSpeechStartupEx(&phTTS, WAVE_MAPPER, REPORT_OPEN_ERROR, MyWndProc, 0);

// Registering messages to report DECtalk asynchronous events

uiID_Error_Message = RegisterWindowMessage("DECtalkErrorMessage");

// Callback message is registered indicating index marks

uiID_Index_Message = RegisterWindowMessage("DECtalkIndexMessage");

// Callback message is registered indicating DECtalk has filled up an audio buffer

uiID_Buffer_Message = RegisterWindowMessage("DECtalkBufferMessage");

}

Related topics