key settings dor Hal and Supernova
==================================

This document is a brief review of the key mapping of Hal and Supernova with Handy Tech 
Braille devices. For this purpose, the function keys on your Braille display correspond 
to Braille dots as follows:
 -  B1 corresponds to Dot 7
 -  B2 corresponds to Dot 3
 -  B3 corresponds to Dot 2 
 -  B4 corresponds to Dot 1 
 -  B5 corresponds to Dot 4 
 -  B6 corresponds to Dot 5
 -  B7 corresponds to Dot 6 
 -  B8 corresponds to Dot 8 


for all Braille devices (except Bookworm)
-----------------------------------------
7             Choose Live Focus  
3             Braille Top  
2             Braille Width Left 
1             Braille Line up  
4             Braille Line down  
5             Braille Width Right  
6             Braille Bottom 
8             Move To Live Focus
2+3           Braille Line Start
5+6           Braille Line End
3+4           Where am I? 
7+8           Physical/Logical Mode  
3+8           Braille Cursor Style 
2+8           Braille Eight Dot Six Dot  
1+8           Handy Tech Configuration Dialog 
4+8           Braille Expand Gaps on off 
5+8           Choose Virtual Focus
6+8           Braille Cycle Attributes
STATUS1       Braille Cycle Attributes 
STATUS2       Braille Verbosity Scheme Cycle            
STATUS3       Braille Tracking on off  
STATUS4       Physical/Logical Mode
1+2+3+4+5+6   Open Control Panel   
1+2+5 [h]     Help 
4+6           Simulate Key Press Tab   
1+3           Simulate Key Press Shift Tab 
1+2+4+5 [g]   Braille Literary Braille on off  
1+3+4 [m]     Simulate Key Press Alt 
2+3+5         Braille Eight Dot Six Dot  
2+3+5+6       List System Tray 
1+3+5+6 [z]   Time & Date
1+4           Simulate Key Press Ctrl Tab  
1+7+4         Simulate Key Press Ctrl Shift Tab  
1+2+3         Simulate Key Press Ctrl Home
4+5+6         Simulate Key Press Ctrl End
1+5 [e]       Simulate Key Press Escape  
2+6           Simulate Key Press Enter
1+2 [b]       Braille Tracking on off
1+2+3+6 [v]   Verbosity Scheme Cycle
1+2+3+5 [r]   reading mode on/off       


for all Braille devices with 16 key pad
---------------------------------------
B9       Physical/Logical Mode  
B10      Braille Cursor Style   
B11      Braille Eight Dot Six Dot  
B12      Handy Tech Configuration Dialog    
B13      Braille Expand Gaps on off 
B14      Choose Virtual Focus 
n0       Simulate Key Press 0   
n1       Simulate Key Press 1   
n2       Simulate Key Press 2   
n3       Simulate Key Press 3   
n4       Simulate Key Press 4   
n5       Simulate Key Press 5   
n6       Simulate Key Press 6   
n7       Simulate Key Press 7   
n8       Simulate Key Press 8 
n9       Simulate Key Press 9


for Modular, Modular Evolution and Easy Braille 
-----------------------------------------------
Left                 Braille Back  
Right                Braille Forward 
Left1+2+3+7          Braille Back
Right4+5+6+8         Braille Forward
Left+Right+1+2+3+7   Braille Line up
Left+Right+4+5+6+8   Braille Line down 
Left+Right           Show or hide status area
Left1+2+7            Braille Input on off  
Right1+2+7           Braille Input on off  


for Modular Evolution
---------------------
Left1+7          ATC on off
Right+1+7        ATC on off
Left+1+2+3       Enables or disables the ATC reading protocol
Right+1+2+3      Enables or disables the ATC reading protocol


for Braille Wave
----------------
Left                 Braille Back
Right                Braille Forward 
Escape               Simulate Key Press Shift Tab  
Enter                Simulate Key Press Tab
Escape+Space+Enter   Show or hide status area  
Space+1+2+7          Braille Input on off

  
for Braille Star 40, 80, Braillino and Modular Evolution
--------------------------------------------------------
TLU/TRU            Braille Back
TLD/TRD            Braille Forward
TLM                Simulate Key Press Shift Tab
TRM                Simulate Key Press Tab 
TLM+TRM            Simulate Key Press Enter


for Braille Star 40, 80 und Braillino
-------------------------------------
SPCL          Braille Back
SPCR          Braille Forward 
SPCL+SPCR     Show or hide status area  
SPCL+1+2+7    Braille Input on off
SPCR+1+2+7    Braille Input on off


for Bookworm
-------------
Backward                  Braille Back  
Forward                   Braille Forward 
Escape                    Choose Live Focus 
Backward+Escape           Choose Virtual Focus
Backward+Enter            Braille Line up 
Forward+Enter             Braille Line down
Backward+Escape+Enter     Braille Line Start
Backward+Escape+Forward   Braille Cursor Style  
Escape+Enter+Forward      Braille Eight Dot Six Dot
Escape+Forward            Braille Cycle Attributes  
Escape+Forward            Go To Focus 
Backward+Forward          Physical/Logical Mode 
Enter                     Routing Button Action 
Backward+Enter+Forward    Open Control Panel of Hal/Supernova



Braille input
=============

- Key combinations are represented by the plus sign "+", e.g. Ctrl+Alt+a. Consecutive 
  key strokes are separated by a comma, e.g. 1, 2 or SPC+123,  z.
- A pressed space key is described with SPC. If a Braille device possesses two space 
  keys, one pressed space key is described with SPC, both pressed space key with SPC2.
- The enter key of a Braille display is described with ENTER, the escape key is 
  described with ESC. With a Braille Star Family device, the left function key is also 
  described with ESC, the right one with ENTER.
- The cursor routing keys are abbreviated as Cr (e.g., Cr12 = cursor routing key above 
  Braille module 12)


all Braille displays
--------------------
SPC+12               Backspace  
SPC+45               Delete 
SPC+24               Insert 
SPC+2345             Tab  
SPC+23457            Back-Tab 
SPC+15               Escape 
SPC+157              Shift-Escape 
SPC+78               Alt for next command 
SPC+36               Ctrl for next command
SPC+3678             AltGr for next command 
SPC+234              Shift for next command 
SPC+2347             Lock Shift 
SPC+1                Cursor up  
SPC+4                Cursor down  
SPC+7                Cursor left  
SPC+8                Cursor right 
SPC+3                Previouse word (CTRL+left) 
SPC+6                Next word (CTRL+right) 
SPC+2                Page up  
SPC+5                Page down  
SPC+13               Home 
SPC+123              Ctrl-Home  
SPC+46               End  
SPC+456              Ctrl-End 
SPC+1234             PAUSE key  
SPC+2456             WIN key  
SPC+24567            Application key  
SPC+24568            WIN key for next command 
SPC                  Space  
SPC+Cr1 ... Cr12     Function keys F1 .. F12  
combination of dots  Character  


for BRW, BL2, BS4, BS8, ME6, ME8
--------------------------------
Enter                Enter  
SPC+Enter            Alt  
Escape               Escape 
Enter+<command>      Alt+<command>  
Escape+<command>     Ctrl+<command> 


for BL2, BS4, BS8, ME6, ME8
---------------------------
SPC2+78              Lock Alt 
SPC2+36              Lock Ctrl
SPC2+3678            Lock AltGr 
SPC2+234             Lock Shift 
SPC2+24568           Lock WIN key 