SAM Driver for Ecobraille Braille display series.

This is a fully functional SAM driver for use with the Ecobraille 40, 80, and Ecoplus Braille displays.

Note: 
The EcoBraille displays don't allow a re-detection of the display once they have been detected. This means that is is necessary that they are switched on just before you try a detection, in case the display was on already switch it off and then back on.
You need to switch the braille display off and on every time you start SAM, do a re-detection in SAM (by pressing "detect all devices now") or start a SAM compatible application (e.g. a Dolphin screen reader).

Please report any bugs to Dolphin. If it crashes please tell us the crash address and registers etc, from the crash message box, also report the driver version number (check with explorer - file properties).


Features
Automatic detection of Braille displays.

Key assignments
The following lists the default keys to press for each Braille operation.
Your screen reader may not support some of these operations. Please refer to the Ecobraille manual for key identifiers.

Action Open Control Panel = F1
Action Open Control Panel = Status Button 2
Braille Back = Left
Braille Forward = Right
Braille Line up = Up
Braille Line up (Virtual Focus) = Up
Braille Line down = Down
Braille Line down (Virtual Focus) = Down
Braille Go To Focus = Shift
Braille Top = Shift + Up
Braille Bottom = Shift + Down
Braille Half Width Left = Shift + Left
Braille Half Width Right = Shift + Right
Braille Physical/Logical Mode = F4
Virtual Focus Physical on off = F4
Braille Literary Braille on off = F3
Braille Cycle Attributes = Status Button 3
Braille Describe Character on off = Status Button 4
Braille Tracking on off = F2
Braille Cursor on off = F5
Braille Eight Dot Six Dot = F8
Braille Layout on off = F6
Braille Verbosity Scheme Cycle = Status Button 1


09/2004