747Pro GPS Trip Recorder 


User’s Manual 

Published on 14-July-2010 V1.3 

Table of Contents 

Chapter 1: Before you begin
1.1: Note and Warning
1.2: Introduction
1.3: Features
1.4: Applications
1.5: Appearance
1.6: Power Switch and Push Button
1.7: LED Display
1.8: Buzzer Alarm
1.9: Vibration sensor for Smart Log


Chapter 2: Getting Started
2.1: Checking the package content
2.2: Getting Started
2.3: Helpful Tips


Appendix


Appendix A. Specifications
Appendix C. Certification 
Appendix D. Warranty Information 


Chapter 1 Before you begin 

1.1 Note and Warning 
- 747Pro uses + Lithium-Ion battery. If 747Pro is used in temperature lower than -10 C° or higher than 60C°, its battery charging capability will decrease. Please leave the 747Pro far from heat or high temperature environment. In addition, do not expose your 747Pro in temperature higher than 140 F°/60C°. If you do not follow these rules, the battery inside 747Pro may overheat, explode or burn itself, and this will lead to very serious damage. The + Lithium-Ion battery inside the 747Pro should be recycled. 

- While in the hospital, turning off the 747Pro is recommended. Wireless GPS receiver may interfere with medical equipments which use radio frequency. 
- For a long period not using 747Pro, take out the battery and store it in dry/cool places. 
- For safety, keep the 747Pro and all accessories out of children’s reach. 
- The manufacturer assumes no responsibility for any damages and loss resulting from the use of this manual, or from deletion of data as a result of malfunction, dead battery, or from misuse of the product in any way. 
- Use only the supplied and approved accessories. Unauthorized accessories, modifications or attachments could damage the 747Pro, and may violate regulations governing radio devices. 
- Use a dry, clean soft cloth to clean the unit. Do not use harsh cleaning solvents, chemicals, or strong detergents. 
- Do not attempt to open the 747Pro yourself. Unauthorized hacking may damage the unit, and void your warranty. 


1.2 Introduction 
This 747Pro logger features an all-in-one, cost-effective portable GPS logging solution. With its on-board memory, it allows you to log your routes by ways of time/ distance/ speed. Points of interest can also be recorded by a push button. With built-in buzzer alarm, 747Pro will beep to let you know GPS location is fixed or a POI is recorded successfully. Through user friendly software utility, it shows your track on Google Earth. This recorder is 
small and robust, ideal to carry everywhere for applications such as route tracking, mountain climbing or fleet management. 


1.3 Features 
1. Dual mode : Data record / Navigation 
2. Push button for POI recording 
3. Smart log of time, distance and speed 
4. Log up to 250,000 waypoints 
5. High receiving sensitivity 
6. AGPS available 
7. Embedded sensor for smart operation 
8. Fuzzy auto on/off 
9. Audio alarm 
10.  Rechargeable battery 
11.  Bluetooth V1.2 compliant 
12.  Photo Tagger software 

1.4 Applications 
-  Record your travels 
-  Manage trip expense 
-  Represent one's driving behavior 
-  Point of Interest recording 
-  Geo-photo support 
-  Show on Google Map & Earth 


1.5 Appearance

1. DC jack (mini USB type): right side
2. Mode switch (Power off/ Navigation/ Navigation&log): left side towards bottom
3. Bluetooth status LED (blue): to the left of the push button 
4. Battery status LED (red/green): to the right of the push button 
5. GPS status LED (orange) / Push to log LED (Red): on top of the push button 
6. Internal GPS antenna 
7. Push Button: raised button in the middle towards the bottom 


1.6 Power Switch and Push Button 
Power Switch 
Right (Off) Power off 
Middle (NAV) Navigation is enabled. 
Left (LOG) Both Navigation & LOG are enabled.
 
Push button
Push: Push button to record POI (Points of Interest), LED will blink 3 times which means the POI is recorded. 


Difference between NAV and LOG: 
NAV Working as a Bluetooth GPS receiver. 
LOG Both of navigation and logging functions are enabled. 

1.7 LED Display 
The 747Pro GPS Trip Recorder has three LED lights, one is Bluetooth Status LED, the 2nd one is Battery Status LED, the 3rd one is GPS Status LED/ Push to log LED. The status table of LED shows as follows: 


Bluetooth Status LED, Color: Blue, Status 1: Always on: Bluetooth on, but not connected to any Bluetooth devices yet. Status 2: Slowly blinking: Sleeping 
mode (1 time / 5 seconds). Status 3: Quickly blinking: Bluetooth is connected and ready for data transmission (1 time / 2 seconds) 

Battery Status LED, Color 1: Red. Status: Blinking: The battery is too low. Color 2: Green. Status 1: Light On: The battery is charging. Status 2: Light Off The battery is fully charged. 

GPS Status LED, Color 1: Orange. Status 1: Always on: Acquiring satellites, GPS position not fixed. Status 2: Quickly Blinking: GPS position is fixed, Navigation. Color 2: Red. Status 1: Quickly Blinking: LED blinks 3 times, Points of Interest is recorded. Status 2: Slowly Blinking The memory space is 
too low (20% left now), Blink 1 time / 5sec. Status 3: Solid on The memory is full and device stops logging.


1.8 Buzzer Alarm 

747Pro is equipped with a buzzer and it supports the alarm by sound. 747Pro will beep as an alarm to let you know when the GPS position is fixed, or when you push the POI button or switch to change to log / navigation mode. 

Beep Descriptions 
Switch to LOG mode = beep (1 sound) 
Switch to NAV mode = beep (1 sound) 
POI recorded = beep~beep~beep (continuous 3 sounds) 
GPS fix = beep~beep (continuous 2 sounds) 
NOTE: When you turn off buzzer by PC software, “Switch” beep alarm still work, only “POI recorded“ and “GPS fix” are disable. 

1.9 Vibration sensor for Smart Log 
747Pro is equipped with a vibration sensor for smart log function. Which means 747Pro can auto detect if itself is static or dynamic. Through this way, 747Pro will stop logging when it detects it is not moving over 5 minutes. And it will wake up and resume to log automatically when it detects it is moving again. 


Chapter 2 Getting Started 

2.1 Checking the package content 
Congratulations on your purchase of the 747Pro with + Lithium-Ion chargeable battery. Before you start using 747Pro, please make sure if your package includes the following items. If any item is damaged or missing, please contact your dealer at once. 

-747Pro GPS Trip Recorder x 1 
-USB to mini-USB cable x 1 
-DC cigarette lighter adapter x 1 
-+ Lithium-Ion chargeable battery x 1 
-CD Tool x 1 (user manual, software utility, driver) 
-Quick start guide x 1 


*. Unit package contents may vary depending on countries without prior notice. 
*. NOTE: The Cigarette Adapter can only be used to charge 747Pro. Please don’t make use of it with devices other than 747Pro. 


2.2 Getting Started 

Please follow the procedure step by step. 

Step 1 Charging Your Battery 
To charge your 747Pro, you have to plug your USB cable into the power source. Charging time is about 3~4 hours and you can charge from PC/ Notebook’s USB 
HOST or from cigarette-lighter in car. 

For the 1st time you use the 747Pro, please charge battery until it is full. The LED that represents the battery is the right-most battery icon (from the push button). 

-If the LED is red, that means battery power is critically low. Charge immediately. 
-If the LED is green, that means battery is charging now. 
-If no LED light display that means battery is fully charged. 


Step 2 Turning on the power switch (NAV/ LOG) 

Power off: No LEDs on
Navigation:  GPS and Bluetooth LEDs on
Data record: Bluetooth LED on 

Difference between NAV and LOG: 
NAV Working as a Bluetooth GPS receiver. 
LOG Both of navigation and logging functions are enabled. 


Step 3 Connecting your handheld device with 747Pro 


Please refer to the user manual of PDA/Smartphone to enable the Bluetooth connectivity. If the connection between your device and 747Pro is successful, 
the blue LED of 747Pro will be blinking. 


Step 4 Loading your GPS mapping or routing software 
You should have mapping software on your PDA/ Smartphone/ laptop or you need to install it before using the 747Pro for navigation. 

Step 5 Starting the application 
Select the correct COM port & baud rate within the application. 
Note: The Bluetooth device in most of the applications has an “auto-detect” feature so that you do not need to select the Baud Rate. 



2.3 Helpful Tips 
-It’s better to turn off the 747Pro when you don’t use it, or the serial Flash's life can’t last long. 
-Some vehicles having heavy metallic sun protecting coating on windshields may affect GPS signal receptions 
-Driving in and around high buildings may affect GPS signal receptions. 
-Driving in tunnels or indoor park may affect signal receptions. 
-In general, any GPS receiver performs best in open space where it can see clean sky. Also weather will affect GPS reception -rain & snow contribute to worse sensitivity. 
-Low battery of a PDA/Smartphone or of an 747Pro may affect signal receptions. 
-Please check the correct “COM” and “Baudrate” of your PDA. 
-747Pro output data updates every second, therefore the actual position and the position shown in your map may have slight time delay. This may happen when 
you drive at higher speed or make a turn around a corner. 
-Note that 747Pro may not work indoors where it can not see the sky. 
-For the 1st time you use the 747Pro, it will take 1 to 3 minutes to obtain the satellite constellation information and fix your position, this is called 
“Cold Start”. If you replace the battery, 747Pro will do Cold Start again. 
-If your 747Pro can’t fix your position for more than 20 minutes, we suggest you change to another spot with open space and then try again. 

Appendix 

Appendix A. Specifications 

General 

Frequency L1,1575.42MHZ 
C/A Code 1.023MHZ 
Datum WGS84 

Performance Characteristics 

Position Accuracy* Without aid: 3.0m 2D-RMS 
<3m CEP(50%) without SA(horizontal) 
DGPS (WAAS,EGNOS,MSAS):2.5m 

Velocity Accuracy* Without aid: 0.1m/s 
DGPS (WAAS,EGNOS,MSAS):0.05m/s 

Acceleration* Without aid:<4g 
DGPS (WAAS,EGNOS,MSAS):<4g 

Timing Accuracy* 50 ns RMS 

Reacquisition Time* <1s 

Hot start* 1.5s 

Warm start* 34s 

Cold start* 35s 

AGPS* <15s 

Sensitivity* Acquisition:-148dBm Max. 
Tracking:-165dBm Max. 

Update* 1Hz 


Dynamic 

Altitude Maximum 18,000m 
Velocity Maximum 515m/s 
Acceleration Maximum 4g 

Power 

Input Voltage Vin : 5.0V±5% 
Battery Chargeable + Lithium-Ion battery 
Operation time 25 hrs 

I/O 

Available Baud Rates 115200 bps 
Protocols NMEA 0183 v3.01 

Environment 

Operating Temperature -10°C ~ +60°C 
Storage Temperature -20°C ~ +80°C 
Charging 0°C ~ +45°C 

Bluetooth 

Standard Fully compliant with Bluetooth V1.2 
Output Power 0dBm (Typical),ClassII 
Range Over 10 meters 
Bluetooth Profile Serial Port Profile(SPP) 
Frequency 2.4G ~ 2.4835GHz ISM Band 
Security Yes 

USB Bridge 

Standard Fully compliant with USB2.0 
Full – speed 12Mbps 
Dimension 46.5 x 72.2 x 20 mm 

Data Log 

64Mbit 
125,000 way points or more 
Log GPS data by time interval/ distance/ speed limit. 
Log GPS data by button push. 
User can configure settings by using utility. 
* Citation MTK original chipset spec. 

Appendix C. Certification FCC Notices 


This device complies with part 15 of the FCC rules. Operation is subject to the following two conditions: 

1. This device may not cause harmful interface, and 
2. This device must accept any interference received, including interference that may cause undesired operation. 

FCC RF Exposure requirements: 
This device and its antenna(s) must not be co-located or operation in conjunction with any other antenna or transmitter. 
NOTE: THE MANUFACTURER IS NOT RESPONSIBLE FOR ANY RADIO OR TV INTERFERENCE CAUSED BY UNAUTHOURIZED MODIFICATION TO THIS EQUIPMENT. SUCH MODIFICATIONS COULD 
VOID THE USER’S AUTHORITY TO OPERATE THE EQUIPMENT. 

CE Notices 


Is herewith confirmed to comply with the requirements set out in the Council Directive on the Approximation of the Laws of the Member States relating to 
Electromagnetic Compatibility (89/336/EEC), Low-voltage Directive (73/23/EEC) and the Amendment Directive (93/68/EEC), the procedures given in European Council Directive 99/5/EC and 89/3360EEC. The equipment was passed. The test was performed according to the following European standards: 


-EN 300 328-2 V.1.2.1 (2001-08) 
-EN 301 489-1 V.1.4.1 (2002-04) / EN 301 489-17 V.1.2.1 (2002-04) 
-EN 50371: 2002 
-EN 60950: 2000 

Appendix D. Warranty Information 

Thank you for your purchase of GPS product from the company. 

The company warrants this product to be free from defects in materials and workmanship for one year from the date of purchase. The warranty for accessories 
is six months. The stamp of distributor or a copy of the original sales receipt is required as the proof of purchase for warranty repairs. The company 
will, as its sole option, repair or replace any components, which fail in normal use. Such repair or replacement will be made at no charge to the customer 
for parts or labor. The customer is, however, responsible for any transportation costs. 
This warranty does not cover failures due to abuse, misuse, accident or unauthorized alteration of repairs. The company assumes no responsibility about products which have been improperly used, abused, damaged due to accident or natural disaster, or damaged due to unauthorized uninstallation, repair 
or modification. 
