		Here's the next revision of the quick reference for the 4500.  This is not a step-by-step how to, you'll need to use the manual to
understand some things and there are most likely some errors.


LG VX4500-4650 Quick Reference - Revision 4 July 17, 2005


LS=Left Soft RS=Right Soft R=Ring L=Left side long key
Options in "()" can be selected via up and down with beep, beep, boop feedback.

Manner mode - Hold * or bottom of L (lid closed)
Keypad Lock - Hold #
Keypad Unlock - RS Your 4 digit PIN (Default is Last 4 digits of phone
number)
Redial - Send Send
Call back last received call - LS 22 Send
Call back last missed call - LS 23 Send
Erase dialed calls - LS 2411
Erase Received calls - LS 2421
Erase missed calls - LS 2431
While in missed calls - RS 51 will erase all
* Does not work from the talking missed calls
* RS 51 also works in Dialed and Received calls
Ringer contact - RS select Contact OK Up 4 times LS R LS
Speed Dial - RS 15 SD# OK Contact OK OK OK
Speed Dial (multiple) - RS 15 SD# OK Contact OK home/mobile/office OK OK

Add contact - Enter phone number then LS, follow prompts
Do not put "1" in front of area codes
The # key is a space and * key is shift
Tap CLR key to erase last character, hold CLR to start over

To edit a contact- RS (contacts),arrow to the contact
you want to change LS (edit).Select to edit hit OK,Hit clear to erase
Type in new info hit OK LS to save.
Contact edit menu starts at the fisrt #. 
Up for name,
Down 
1 =new #,The following down #'s will increase for every # added.
2 = email
3 = Group
4 = ringer

Record memo - LS 72 LS
Play last memo - LS 72 OK LS
Start/Stop memo playback - LS
Pause/Resume memo - RS (while memo is playing)
Delete memo while playback - LS RS 21
Next memo while playback - LS R LS
Erase all memos - LS 72 RS 41

Alarms - LS 81 (A1 A2 A3 QuickTimer)
Alarm A1 - LS 811 (OnOff Time Occurrence Ringer)
Alarm on/Off - LS 811 OK down (Beep=Off Boop=On
Alarm Time - LS 811 down OK hhmm AM/PM 
Press LS to save alarm 
After OK on time the Occurrence is highlighted
Alarm Occurrence - LS 811 Down Down OK 
Alarm Occurrence (Once EveryDay Weekdays Weekends)
Alarm Ringer - LS 811 up OK ringer  
QuickTimer - LS 814 (10min 30min 1hr 3hr)

Scheduler - LS 82
New appointment - LS 82  (Date Time Note VM Occurrence OnTime Ringer) LS to
save
Date can be entered as mmddyyyy
Time can be entered as hhmm, defaults to current time
Note - Skip it, doesn't speak
Voice Memo - OK to start recording, LS to stop
When you press LS to stop recording the Occurrence will be highlighted.
Occurrence (once daily weekdays weekly monthly yearly)
OnTime (OnTime 5Min 10min 1hr 1day 2days none)
The OnTime is used to notify you before the event.
Ringer - Notification ring

Today's appointments - LS 82 OK OK
The First OK opens the appointment list for this day.
The Second OK plays the voice memo 
Left / Right to move through all appointments for this date while playing
Tomorrow's appointments - LS 82 Right OK OK
Appointment week from Today - LS 82 Down OK OK
Edit appointment - LS while on the appointment
Erase appointment - RS 21 on appointment 
Erase all appointments on selected date - RS 31

Ringers
Caller ID - LS 9111 then select (up/down), save with OK
No Caller ID - LS 9112 then select (up/down), save with OK
Restrict (caller ID Blocked by caller)- LS 9113 then select (up/down),  save with OK
Key Tone length (vx4500) - LS 912 (Normal, Long) OK
Key Tone or speech (vx4650) - LS 912 (beep, english, spanish) OK

Volumes 
Ringer - LS 9131 (low, med low, med, med high, high, vibrate and high) OK
When ringer volume is max phone either rings and vibrates or caller id and vibrates. 
Earpiece - LS 9132 (low, med low, med, med high, high) OK			
Key beep - LS 9133 (off, low, med low, med, med high, high) OK
Speakerphone - LS 9134 (low, med low, med, med high, high) OK

Setting Alerts 
Service alert - LS 9141 (on, off) OK
Minute beep - LS 9142 (on, off) OK
Call connect tones - LS 9143 (on, off) OK 
Back to top (Beep/Beep/Boop option) - LS 9144 (on, off) OK
ERI Cell Service Status - LS 9145 (on, off) OK

Power ON/Off tones - LS 915 (on, off) OK
Banner - LS 921 enter text OK
Backlight timer - LS 922 OK OK (7s, 15s, 30s, Always on, Always off) OK
Backlight brightness - LS 92 OK 2 (0%, 25%, 50%, 75%, 100%) use left or right of R to select OK
Key Light timer - LS 9222 (7s, 15s, 30s, Always ON, Always Off, Brightness) OK

Lock mode - LS 94 Your 4 digit pin 1 (Unlock, Lock, Lock on Powerup) 
Restrict - LS 94 Your 4 digit pin 2 (On, Off) 
Emergency #'s - LS 94 Your 4 digit pin 3 (911, 611, *611)
GPS Location support - LS 97 (Location on, E911 only) OK 
Reset to Factory defaults - LS 94 4 digits of PIN 6 OK Up once OK
 

