#AJB

,,MIDI ,,FUNC;NS

,! ,PORTA,T"O IS ,,MIDI,'-COMPATI#1

F1TUR+ ,,MIDI ,,9 & ,,MIDI ,,\ T]M9ALS &

PROVID+ A V>IETY ( ,,MIDI-RELAT$ 3TROLS4

,0US+ ! ,,MIDI FUNC;NS Y C EXP& YR

MUSICAL POSSIBILITIES4 ,? SEC;N EXPLA9S

:AT ,,MIDI IS1 & :AT X C D1 Z WELL Z H[

Y C USE ,,MIDI ON YR ,,PSR-#CDJ4

,,IMPORTANT3

,! ,,MIDI FUNC;NS _C 2 US$ 9 ! ,S;G

MODE4

,,:AT ,,IS ,,MIDI8

,NO D\BT Y H HE>D ! T]MS AC\/IC 9/RU;T &

DIGITAL 9/RU;T4 ,9 ! _W TD1 ^! >E ! TWO

MA9 CATEGORIES ( 9/RU;TS4 ,LET'S 3SID]

AN AC\/IC PIANO &A CLASSICAL GUIT> Z

REPRES5TATIVE AC\/IC 9/RU;TS4 ,!Y >E

EASY 6"U/&4 ,)! PIANO1 Y /RIKE A KEY1 &A

HAMM] 9SIDE HITS "S /R+S & PLAYS A NOTE4

,)! GUIT>1 Y DIRECTLY PLUCK A /R+ &!

NOTE S.DS4 ,B H[ DOES A DIGITAL 9/RU;T G

AB PLAY+ A NOTE8 A#AJB

,Z %[N 9 ! ILLU/R,N ABV1 9 AN

ELECTRONIC 9/RU;T ! SAMPL+ NOTE

7PREVI\SLY RECORD$ NOTE7 /OR$ 9 ! T"O

G5]ATOR SEC;N 7ELECTRONIC CIRCUIT7 IS

PLAY$ BAS$ ON 9=M,N RCVD F ! KEYBO>D4 ,S

!N :AT IS ! 9=M,N F ! KEYBO>D T 2COMES !

BASIS = NOTE PRODUC;N8

,= EXAMPLE1 LET'S SAY Y PLAY A ;,C

QU>T] NOTE US+ ! GR& PIANO S.D ON !

,,PSR-#CDJ KEYBO>D4 ,UNLIKE AN AC\/IC

9/RU;T T PUTS \ A RESONAT$ NOTE1 !

ELECTRONIC 9/RU;T PUTS \ 9=M,N F !

KEYBO>D S* Z 8) :AT VOICE10 8) : KEY10

8AB H[ /R;G10 8:5 0 X PRESS$10 & 8:5 0 X

REL1S$40 ,!N EA* PIECE ( 9=M,N IS *ANG$

96A NUMB] VALUE & S5T 6! T"O G5]ATOR4

,US+ ^! NUMB]S Z A BASIS1 ! T"O G5]ATOR

PLAYS ! /OR$ SAMPL+ NOTE4

,EXAMPLE ( ,KEYBO>D ,9=M,N

,VOICE NUMB] 7) :AT VOICE73 #JA 7GR&

PIANO7

,NOTE NUMB] 7) : KEY73 #FJ 7,C#C7

,NOTE ON 7:5 0 X PRESS$7 & NOTE (F 7:5

0 X REL1S$73 ,TIM+ EXPRESS$ B#AJB

NUM]IC,Y 7QU>T] NOTE7

,VELOC;Y 7AB H[ /R;G73 #ABJ 7/R;G7

------------------------------------#AJC

,,MIDI IS AN ACRONYM T /&S = ,MUSICAL

,9/RU;T ,DIGITAL ,9T]FACE1 : ALL[S

ELECTRONIC MUSICAL 9/RU;TS 6-MUNICATE )

EA* O!R1 0S5D+ & RCVG -PATI# ,NOTE1

,3TROL ,*ANGE1 ,PROGRAM ,*ANGE & V>I\S

O!R TYPES ( ,,MIDI DATA1 OR MESSAGES4 ,!

,,PSR-#CDJ C 3TROL A ,,MIDI DEVICE

0TRANSMITT+ NOTE RELAT$ DATA & V>I\S

TYPES ( 3TROLL] DATA4 ,! ,,PSR-#CDJ C 2

3TROLL$ 0! 9COM+ ,,MIDI MESSAGES :

AUTOMATIC,Y DET]M9E T"O G5]ATOR MODE1

SELECT ,,MIDI *ANNELS1 *ANGE P>AMET]

VALUES &( C\RSE PLAY ! VOICES SPECIFI$

=! V>I\S "PS4

,,MIDI MESSAGES C 2 DIVID$ 96TWO

GR\PS3 ,*ANNEL MESSAGES & ,SY/EM

MESSAGES4 ,2L IS AN EXPLAN,N (! V>I\S

TYPES ( ,,MIDI MESSAGES : ! ,,PSR-#CDJ C

RCV/TRANSMIT4

,*ANNEL ,MESSAGES A#AJC

,! ,,PSR-#CDJ IS AN ELECTRONIC 9/RU;T T

C H&LE #AF *ANNELS4 ,? IS USU,Y EXPRESS$

Z X C PLAY #AF 9/RU;TS AT ! SAME "T4

,*ANNEL MESSAGES TRANSMIT 9=M,N S* Z

,NOTE ,,ON/,,(F1 ,PROGRAM ,*ANGE1 = EA*

(! #AF *ANNELS4

,',! FOLL[+ TA# HAS TWO COLUMNS H1D$

8,MESSAGE ,"N0 & 8,,PSR-#CDJ

,OP],N/,PANEL ,SETT+04,'

,NOTE ,ON/,(F

,MESSAGES : >E G5]AT$ :5 ! KEYBO>D IS

PLAY$4 ,EA* MESSAGE 9CLUDES A SPECIFIC

NOTE NUMB] : CORRESPONDS 6! KEY : IS

PRESS$1 PLUS A VELOC;Y VALUE BAS$ ON

H[ H>D ! KEY IS /UCK4

,PROGRAM ,*ANGE

,VOICE NUMB] 7AL;G ) CORRESPOND+ BANK

SELECT ,,MSB/,,LSB SETT+S1 IF NEC74

,3TROL ,*ANGE

,MESSAGES T >E US$ 6*ANGE "S ASPECT (!

S.D 7MODUL,N1 VOLUME1 PAN1 ETC474

,SY/EM ,MESSAGES B#AJC

,? IS DATA T IS US$ 9 -MON 0! 5TIRE

,,MIDI SY/EM4 ,SY/EM MESSAGES 9CLUDE

MESSAGES L ,EXCLUSIVE ,MESSAGES T

TRANSMIT DATA UNIQUE 6EA* 9/RU;T

MANUFACTUR] & ,R1L"T ,MESSAGES T 3TROL !

,,MIDI DEVICE4

,',! FOLL[+ TA# HAS TWO COLUMNS H1D$

8,MESSAGE ,"N0 & 8,,PSR-#CDJ

,OP],N/,PANEL ,SETT+04,'

,EXCLUSIVE ,MESSAGE

,REV]B/*ORUS/,,DSP SETT+S1 ETC4

,R1L"T ,MESSAGES

,CLOCK SETT+ ,/>T//OP OP],N

,! MESSAGES TRANSMITT$/RCVD 0! ,,PSR-

#CDJ >E %[N 9 ! ,,MIDI ,IMPLE;T,N ,*>T

ON PAGE #ABJ4

,,MIDI ,T]M9ALS

,9 ORD] 6EX*ANGE ,,MIDI DATA 2T MULTIPLE

DEVICES1 EA* DEVICE M/ 2 3NECT$ 0A CA#4

,! ,,MIDI T]M9ALS (! ,,PSR-#CDJ >E

LOCAT$ ON ! RE> PANEL4 C#AJC

,,MIDI ,,IN3 ,RCVS ,,MIDI DATA F ANO!R

,,MIDI DEVICE4

,,MIDI ,,\3 ,TRANSMITS ! ,,PSR-#CDJ'S

KEYBO>D 9=M,N Z ,,MIDI DATA 6ANO!R

,,MIDI DEVICE4

,NOTE3

99 ,SPECIAL ,,MIDI CA#S 7SOLD SEP>ATELY7

M/ 2 US$ = 3NECT+ 6,,MIDI DEVICES4

,!Y C 2 B"\ AT MUSIC /ORES ETC4

99 ,N"E USE ,,MIDI CA#S L;G] ?AN AB #AE

MET]S4 ,CA#S L;G] ?AN ? C PICK UP

NOISE : C CAUSE DATA ]RORS4

------------------------------------#AJD

,,:AT ,,Y ,,C ,,D ,,) ,,MIDI

,! ,,PSR-#CDJ AL F1TURES RE> PANEL

,,MIDI T]M9ALS 7,,MIDI ,,9 & ,,MIDI ,,\7

Z WELL Z A -PREH5SIVE SET ( ,,MIDI

FUNC;NS1 T LET Y USE ! 9/RU;T 9 A V>IETY

( RECORD+ & P]=M.E APPLIC,NS4

99 ,3TROLL+ ! ,,PSR-#CDJ )A ,,MIDI

KEYBO>D 3TROLL] 7N HAV+ A T"O

G5]ATOR7 7,AUTO A3OMPANI;T C AL 2 US$

9 ? SETUP47 A#AJD

99 ,9 ? SETUP Y C RECORD YR ,,PSR-#CDJ

P]=M.E1 9CLUD+ ! AUTO A3OMPANI;T1 6A

3NECT$ -PUT] OR SEQU;ER4 7,UP 6#AF

*ANNELS C 2 US$47 ,Y C !N $IT !

RECORD$ DATA ON ! -PUT] OR SEQU;ER1 &

PLAY X BACK US+ ! S.DS (! ,,PSR-#CDJ4

,NOTE3 ,:5 US+ A P]SONAL -PUT]1 SPECIAL

S(TW>E 7SEQU;ER S(TW>E7 IS NE$$4

------------------------------------#AJE

,,3NECT+ ,,6,A ,,P]SONAL ,,-PUT]

,03NECT+ YR ,,PSR-#CDJ'S ,,MIDI T]M9ALS

6A P]SONAL -PUT]1 Y C H A3ESS 6A WIDE

V>IETY ( MUSIC S(TW>E4

,:5 US+ A ,,MIDI 9T]FACE DEVICE 9/ALL$

9 ! P]SONAL -PUT]1 3NECT ! ,,MIDI

T]M9ALS (! P]SONAL -PUT] &! ,,PSR-#CDJ4

,USE ONLY SPECIAL ,,MIDI CA#S :5

3NECT+ ,,MIDI DEVICES4

99 ,3NECT ! ,,MIDI T]M9ALS (! ,,PSR-#CDJ

6! ,,MIDI T]M9ALS (! P]SONAL -PUT]4

99 ,:5 US+ A ,,MIDI 9T]FACE )A ,MAC9TO%

S]IES -PUT]1 3NECT ! ,,RS-#DBB T]M9AL

(! -PUT] 7MODEM OR PR9T] A#AJE

T]M9AL7 6! ,,MIDI 9T]FACE1 Z %[N 9 !

DIAGRAM 2L4

,NOTE3 ,:5 US+ A ,MAC9TO% S]IES -PUT]1

SET ! ,,MIDI 9T]FACE CLOCK SETT+ 9 !

APPLIC,N S(TW>E 6MAT* ! SETT+ (! ,,MIDI

9T]FACE Y >E US+4 ,= DETAILS1 C>E;LLY

R1D ! [N]'S MANUAL =! S(TW>E Y >E US+4

------------------------------------#AJF

,,FUNC;N ,,P>AMET]S--,,MIDI

,! ,FUNC;N P>AMET]S PROVIDE A4I;NAL1 M

DETAIL$ ,,MIDI SETT+S =! ,PORTA,T"O4 ,^!

SETT+S 9CLUDE3

99 ,REMOTE ,*ANNEL

99 ,KEYBO>D ,\

99 ,A3OMPANI;T ,\

99 ,LOCAL ,3TROL

99 ,EXT]NAL CLOCK

99 ,9ITIAL ,SETUP ,S5D

#A ,CALL UP ! ,FUNC;N MODE4

,PRESS ! ,,FUNC;N BUTTON4

#B ,SELECT ! DESIR$ ,FUNC;N P>AMET]4

,:ILE ! 8,,FUNC;N0 9DIC,N IS A#AJF

FLA%+1 USE ! NUM]IC KEYPAD 6SELECT !

DESIR$ ,,MIDI ,FUNC;N P>AMET] NUMB]

7#HA-HG74 7,SEE ! ,P>AMET]S LI/ 2L =

DETAILS47

,FUNC;N P>AMET] NUMB]S C 2 SELECT$

9 ! SAME WAY Z )! VOICES 7SEE PAGE

#BH7 )! NUM]IC KEYPAD1 ;6/;- KEYS1 OR

! ,,FUNC;N BUTTON4

,IMPORTANT3 ,S9CE ! 8,,FUNC;N0

9DIC,N FLA%ES = ONLY A C\PLE (

SECONDS1 MAKE SURE 6SELECT ! P>AMET]

QKLY AF /EP #A ABV4

#C ,*ANGE ! P>AMET] SETT+ OR VALUE4

,AF ! 8,,FUNC;N0 9DIC,N /OPS FLA%+1

USE ! NUM]IC KEYPAD 6*ANGE ! VALUE OR

SETT+4

,RE/OR+ ! ,DEFAULT ,VALUE3 ,IF Y'VE

*ANG$ ! P>AMET] SETT+1 Y C 9/ANTLY

RE/ORE ! DEFAULT SETT+ 0PRESS+ BO?

;6/;- BUTTONS SIMULTANE\SLY4

,NOTE3 ,! ,,MIDI SETT+S 2L >E SAV$

EV5 :5 ! P[] IS TURN$ (F4 ,H["E1

,,MIDI SETT+S >E ,,N 9CLUD$ 9 ! DATA

SAV$ 6! ,US] BANKS 9 ! ,"O ,T\*

,SETT+ F1TURE 7PAGE #GB74 B#AJF

#D ,SET O!R P>AMET]S Z NE$$4

,6SELECT & SET O!R P>AMET]S1 REP1T

/EPS #A-C ABV4

#E ,EXIT ! ,FUNC;N MODE4

,ONCE Y'VE MADE ALL DESIR$ SETT+S1

PRESS "O (! O!R MODE BUTTONS 7,,S;G1

,,/YLE1 OR ,,VOICE74

------------------------------------#AJG

,FUNC;N ,P>AMET]S

,',! FOLL[+ TA# HAS F\R COLUMNS H1D$

8,NO401 8,P>AMET] ,"N01 8,4PLAY ,"N01 &

8,RANGE/,SETT+S04 ,"! IS AL A DESCRIP;N

( EA* ITEM4,'

#HA

,REMOTE ,*ANNEL

,REMOTE,CH

(F1 #JA-AF

,? DET]M9ES H[ ! ,PORTA,T"O IS

3TROLL$ 0A REMOTE 7EXT]NAL7

,,MIDI KEYBO>D4 ,SET ? 6"O (!

#AF *ANNELS 7#JA-AF7 = US+ AN

EXT]NAL KEYBO>D 6REMOTELY 3TROL

! ,PORTA,T"O FUNC;NS OV] A#AJG

! SELECT$ *ANNEL4 7,! REMA9+ #AE

*ANNELS C 2 US$ = MULTI-TIMBRAL

OP],N47 ,:5 ? IS SET TO 8(F10 !

,PORTA,T"O C 2 US$ Z A FULL #AF-

*ANNEL MULTI-TIMBRAL S.D S\RCE4

,! DEFAULT SETT+ IS 8(F40

#HB

,KEYBO>D ,\

,KBD,\T

ON/(F

,? DET]M9ES :E!R ! KEYBO>D

P]=M.E DATA (! ,PORTA,T"O IS

TRANSMITT$ OR N4 ,:5 ? IS SET TO

8(F10 NOTES PLAY$ ON !

,PORTA,T"O W N A6ECT 7N 2

TRANSMITT$ TO7 ! 3NECT$ ,,MIDI

DEVICE4 ,:5 ? IS SET TO 8ON10 !

FOLL[+ KEYBO>D DATA IS

TRANSMITT$3 ,MA9 VOICE "P OV]

*ANNEL #A1 ,SPLIT VOICE "P OV]

*ANNEL #B1 & ,DUAL VOICE "P OV]

*ANNEL #AA4 ,! DEFAULT SETT+ IS

8ON40

,NOTE3 ,IF BO? ,KEYBO>D ,\ &

,LOCAL ,3TROL 7#HD 2L7 B#AJG

>E SET TO 8(F10 NEI ! 3NECT$

,,MIDI DEVICE NOR ! ,PORTA,T"O

VOICES W S.D :5 PLAY+ ! KEYBO>D4

#HC

,A3OMPANI;T ,\

,ACMP,\T

ON/(F

,? DET]M9ES :E!R ,AUTO

,A3OMPANI;T DATA IS TRANSMITT$

VIA ,,MIDI ,,\ OR N4 ,:5 SET TO

8ON10 ,AUTO ,A3OMPANI;T DATA IS

TRANSMITT$ OV] *ANNELS #C-AJ 7Z

LI/$ 2L74 ,! DEFAULT SETT+ IS

8ON40

,A3OMPANI;T ,TRANSMIT ,*ANNELS3

,*ANNEL #C--,BASS

,*ANNEL #D--,*ORD "P #A

,*ANNEL #E--,*ORD "P #B

,*ANNEL #F--,PAD

,*ANNEL #G--,PHRASE "P #A

,*ANNEL #H--,PHRASE "P #B

,*ANNEL #I--,RHY?M "P #B

,*ANNEL #AJ--,RHY?M "P #A

,H9T3 ,Y C USE ,A3OMPANI;T ,\ 9

S"EAL WAYS4 ,"O USE;L C#AJG

APPLIC,N WD 2 6PLAY ALL OR

SELECT$ "PS ON A 3NECT$ ,,MIDI

T"O G5]ATOR4 ,9 ? WAY Y CD

RE9=CE ! ,PORTA,T"O S.DS 0LAY]+

7OR SUB/ITUT+7 )! S.DS (! T"O

G5]ATOR4 ,9 A DI6]5T APPLIC,N1 Y

CD RECORD ! 9DIVIDUAL "PS F EA*

*ANNEL 6A SEQU;ER1 & USE !

-PREH5SIVE $IT+ F1TURES (!

SEQU;ER 6RE>RANGE ! A3OMPANI;T

"PS4

#HD

,LOCAL ,3TROL

,LOCAL

ON/(F

,? DET]M9ES :E!R ! KEYBO>D IS

3NECT$ 6! 9T]NAL ,VOICES (!

,PORTA,T"O4 ,:5 SET TO 8ON10 !

,VOICES RESPOND 6NOTES PLAY$ F !

KEYBO>D4 ,:5 SET TO 8(F10 !

,VOICES RESPOND ONLY 69COM+

,,MIDI DATA 7VIA ,,MIDI ,,IN74

,! DEFAULT SETT+ IS 8ON40 ,IF Y

>E R\T+ ! ,,MIDI ,,\ ON !

,PORTA,T"O 6A SEQU;ER & D#AJG

BACK 6! ,,MIDI ,,IN1 Y MAY WANT

6SET ? TO 8(F0 6AVOID ,,MIDI

FE$BACK4

------------------------------------#AJH

#HE

,EXT]NAL ,CLOCK

,EXT,CLOCK

ON/(F

,? DET]M9ES :E!R ! /YLE & S;G

PLAYBACK FUNC;NS >E 3TROLL$ 0!

,PORTA,T"O'S 9T]NAL CLOCK 7(F7

OR 0,,MIDI CLOCK DATA F AN

EXT]NAL SEQU;ER OR -PUT] 7ON74

,? %D 2 SET TO 8ON0 :5 Y WANT 6H

/YLE OR S;G PLAYBACK FOLL[ !

EXT]NAL DEVICE 7S* Z A RHY?M

MA*9E OR A SEQU;ER74 ,! DEFAULT

SETT+ IS 8(F40

,NOTE3 ,:5 ? IS SET TO 8ON10

/YLE PLAYBACK ,,_C 2 3TROLL$ F !

,PORTA,T"O PANEL 3TROLS4

,EXT]NAL ,CLOCK IS AUTOMATIC,Y

SET TO 8(F0 :5 ! ,S;G MODE IS

SELECT$4

#HF A#AJH

,9ITIAL ,SETUP ,S5D

,9IT,S5D

----

,? FUNC;N LETS Y TRANSMIT !

9ITIAL SETUP SETT+S (!

,PORTA,T"O 6A SEQU;ER & RECORD

!M Z "P (A S;G4 ,? 5SURES T :5 Y

PLAYBACK ! S;G1 ! ,PORTA,T"O IS

9/ANTLY & AUTOMATIC,Y

RECONFIGUR$ 6! PROP] SETT+S =!

S;G4 7,= DETAIL$ 9/RUC;NS1 SEE !

SEC;N 8,,US+ ,,9ITIAL ,,SETUP

,,S5D ,,) ,A ,,SEQU;ER0 2L47

,US+ ,9ITIAL ,SETUP ,S5D )A ,SEQU;ER

,! MO/ -MON USE =! ,9ITIAL ,SETUP ,S5D

FUNC;N IS 9 RECORD+ A S;G ON A SEQU;ER T

IS 9T5D$ = PLAYBACK )! ,PORTA,T"O4

,ESS5TI,Y1 ? TAKES A SNAP%OT (!

,PORTA,T"O SETT+S & S5DS T DATA 6!

SEQU;ER4 ,0RECORD+ ? SNAP%OT AT ! />T (!

S;G 72F ANY ACTUAL P]=M.E DATA71 Y C

9/ANTLY RE/ORE ! NEC SETT+S ON !

,PORTA,T"O4 ,PROVID$ "! IS A PAUSE 9 !

S;G1 Y CD AL D ? 9 ! MI4LE (A B#AJH

S;G--= EXAMPLE1 -PLETELY *ANG+ !

,PORTA,T"O SETT+S =! NEXT SEC;N (! S;G4

,S5D+ ,9ITIAL ,SETUP ,DATA

#A ,F/1 SET UP ! SEQU;ER = RECORD+4

,! ACTUAL PROC$URE MAY DI6] DEP5D+ ON

YR "PICUL> EQUIP;T & S(TW>E4

,IDE,Y1 Y %D L1VE TWO OR M M1SURES

( SIL;E 7NO P]=M.E DATA7 2F ! S;G

2G9S4 ,! ,9ITIAL ,SETUP DATA %D !N 2

RECORD$ 6? SPACE 9 ! S;G4

------------------------------------#AJI

#B ,ON ! ,PORTA,T"O1 SELECT ! ,9ITIAL

,SETUP ,S5D FUNC;N4

,D ? 9 ! NORMAL WAY3

#A7 ,PRESS ! ,,FUNC;N BUTTON4

#B7 ,SELECT P>AMET] #HF 7)! NUM]IC

KEYPAD74

#C ,AT ! 8,9IT,SND80 PROMPT ABV1 SET !

OP],N 6/&BY4

,PRESS ! ;6 BUTTON4

#D ,/>T RECORD+ ON ! SEQU;ER1 !N S5D !

,9ITIAL ,SETUP DATA4

,/>T RECORD+ ON ! SEQU;ER 9 ! NORMAL

WAY1 !N ) Z LL DELAY Z POSSI# A#AJI

PRESS ! ;6 BUTTON 6ACTU,Y />T

TRANSMITT+ ! DATA4

,AN 8,5D0 MESSAGE BRIEFLY APPE>S 9

! 4PLAY :5 ! OP],N IS -PLETE1 FOLL[$

0! 8,9IT,SND80 PROMPT4

#E ,/OP RECORD+ ON ! SEQU;ER4

,/OP RECORD+ ON ! SEQU;ER 9 ! NORMAL

WAY4 ,MAKE SURE T ANY SUBSEQU5TLY

RECORD$ P]=M.E DATA IS RECORD$ AT L1/

"O M1SURE FOLL[+ ! ,9ITIAL ,SETUP

DATA4

#F ,EXIT F ! ,9ITIAL ,SETUP ,S5D OP],N4

,6EXIT F ,9ITIAL ,SETUP ,S5D1 PRESS

"O (! O!R MODE BUTTONS3 ,,S;G1

,,/YLE1 OR ,,VOICE4