#AAJ

,,TR\#%OOT+

,',! FOLL[+ TA# HAS TWO COLUMNS H1D$

8,PRO#M0 & 8,POSSI# ,CAUSE & ,SOLU;N04,'

,:5 ! ,PORTA,T"O IS TURN$ ON OR (F1 A

POPP+ S.D IS TEMPOR>ILY PRODUC$4

,? IS NORMAL & 9DICATES T ! ,PORTA,T"O

IS RCVG ELECTRICAL P[]4

,:5 US+ A MOBILE PH"O1 NOISE IS PRODUC$4

,US+ A MOBILE PH"O 9 CLOSE PROXIM;Y 6!

,PORTA,T"O MAY PRODUCE 9T]F];E4

,6PREV5T ?1 TURN (F ! MOBILE PH"O OR

USE X FUR!R AWAY F ! ,PORTA,T"O4

,"! IS NO S.D EV5 :5 ! KEYBO>D IS PLAY$

OR :5 A S;G IS 2+ PLAY$ BACK4

,*ECK T NO?+ IS 3NECT$ 6!

,,PH"OS/,,\TPUT JACK ON ! RE> PANEL4

,:5 A SET ( H1DPH"OS IS PLU7$ 96?

JACK1 NO S.D IS \TPUT4

,! SELECT$ VOICE DOES N S.D PROP]LY1 OR

IS TOO L[ 9 VOLUME4

,MAKE SURE T ! FOLL[+ SETT+S >E

APPROPRIATE3 ,MA9 ,VOICE ,VOLUME 7#JA1

PAGE #CA71 ,DUAL ,VOICE A#AAJ

,VOLUME 7#AA1 PAGE #CE71 & ,SPLIT

,VOICE ,VOLUME 7#BA1 PAGE #CG74

,"! IS NO S.D :5 PLAY+ ! KEYBO>D4

,:5 SETT+ ! ,SPLIT ,PO9T1 ! KEYBO>D IS

US$ ONLY 6*ANGE ! VALUE & DOES N

PRODUCE ANY S.D4

,PLAY+ KEYS 9 ! "R H& SEC;N (! KEYBO>D

DOES N PRODUCE ANY S.D4

,:5 US+ ! ,DIC;N>Y TYPE 7,*ORD ,GUIDE1

PAGE #FB71 ! KEYS 9 ! "R H& SEC;N >E

US$ ONLY = 5T]+ ! *ORD ROOT & TYPE4

,! S.D (! VOICES OR RHY?MS SEEMS UNUSUAL

OR /RANGE4

,! BATT]Y P[] IS TOO L[4 ,REPLACE !

BATT]IES4 7,SEE PAGE #H47

,! A3OMPANI;T DOES N PLAY BACK EV5 :5

PRESS+ ! ,,/>T/,,/OP BUTTON4

,:5 ,EXT]NAL ,CLOCK 7PAGE #AJH7 IS SET

TO 8ON10 /YLE PLAYBACK ,,_C 2 3TROLL$

F ! ,PORTA,T"O PANEL 3TROLS4

,"! IS NO S.D ON EI ! ,PORTA,T"O OR !

3NECT$ ,,MIDI DEVICE4

99 ,IF ,LOCAL ,3TROL 7,FUNC;N #HD1

PAGE #AJG7 IS SET TO 8(F10 !

,PORTA,T"O VOICES W N S.D B#AAJ

EV5 :5 PLAY+ ! KEYBO>D4

99 ,IF ,KEYBO>D ,\ 7,FUNC;N #HB1 PAGE

#AJG7 IS SET TO 8(F10 ! 3NECT$

,,MIDI DEVICE W N S.D :5 PLAY+ !

,PORTA,T"O KEYBO>D4

,! A3OMPANI;T DOES N S.D PROP]LY4

99 ,MAKE SURE T ! ,A3OMPANI;T ,VOLUME

7PAGE #EE7 IS SET 6AN APPROPRIATE

LEVEL4

99 ,MAKE SURE T ! ,A3OMPANI;T ,SPLIT

,PO9T 7#EA1 PAGE #EI7 IS SET 6AN

APPROPRIATE VALUE4

,! ,REV]B/,*ORUSST,,DSP/,H>MONY _C 2

HE>D PROP]LY4

99 ,MAKE SURE T ! ,S5D ,LEVEL P>AMET]

=! E6ECT 7&! 9T5D$ VOICE3 ,MA91

,DUAL1 OR ,SPLIT7 IS SET 6AN

APPROPRIATE VALUE4 7,SEE PAGES #CA1

#CE1 #CG7

99 ,MAKE SURE T ! CORRESPOND+ E6ECT IS

TURN$ ON4 7,SEE PAGES #DJ1 #DA1

#DB1 #DC7

99 ,=! ,H>MONY E6ECT1 MAKE SURE T

,H>MONY ,VOLUME 7#CI1 PAGE #DD7 IS

SET 6AN APPROPRIATE VALUE4 C#AAJ

,:5 PLAY+ BACK "O (! ,PIANI/ /YLES 7#IA-

AJJ71 ! RHY?M _C 2 HE>D4

99 ,? IS NORMAL4 ,! ,PIANI/ /YLES H NO

DRUMS OR BASS--ONLY PIANO

A3OMPANI;T4 ,! A3OMPANI;T (! /YLE C

ONLY 2 HE>D :5 A3OMPANI;T IS SET

6,,ON & KEYS >E PLAY$ 9 ! AUTO

A3OMPANI;T SEC;N (! KEYBO>D4

,N ALL (! VOICES SEEM 6S.D1 OR ! S.D

SEEMS 6BE CUT (F4

,! ,PORTA,T"O IS POLYPHONIC UP 6A

MAXIMUM ( #CB NOTES4 ,IF ! ,DUAL

VOICE OR ,SPLIT VOICE MODE IS 2+

US$ &A /YLE OR S;G IS PLAY+ BACK AT

! SAME "T1 "S NOTES/S.DS MAY 2

OMITT$ 7OR /OL57 F ! A3OMPANI;T OR

S;G4 7,SEE ! NOTE ON PAGE #AAD47

------------------------------------#AAA

,A /RANGE FLANG+ OR D\BL+ S.D O3URS :5

US+ ! ,PORTA,T"O )A SEQU;ER4 7,? MAY

AL S.D L A DUAL LAY]$ S.D ( TWO

VOICES1 EV5 :5 ,DUAL IS TURN$ (F47

99 ,IF Y >E R\T+ ! ,,MIDI ,,\ ON !

,PORTA,T"O 6A SEQU;ER & BACK 6!

,,MIDI ,,IN1 Y MAY WANT A#AAA

6SET ,LOCAL ,3TROL 7PAGE #AJG7 TO

8(F0 6AVOID ,,MIDI FE$BACK4

99 ,:5 US+ ! A3OMPANI;T )A SEQU;ER1

SET ,,MIDI ,E*O 7OR ! RELEVANT

3TROL7 TO 8(F40 7,REF] 6! [N]'S

MANUAL ( YR "PICUL> DEVICE &/OR

S(TW>E = DETAILS47

,! FOOTSWIT* SEEMS 6PRODUCE ! OPPOSITE

E6ECT4 ,= EXAMPLE1 :5 US+ ! FOOTSWIT* =

SU/A91 PRESS+ ! FOOTSWIT* CUTS (F ! S.D

& REL1S+ X SU/A9S ! S.DS4

,! POL>;Y (! FOOTSWIT* IS REV]S$4

,MAKE SURE T ! FOOTSWIT* PLUG IS

PROP]LY 3NECT$ 6! ,,FOOT ,,SWIT* JACK

2F TURN+ ON ! P[]4

,! S.D (! VOICE *ANGES F NOTE 6NOTE4

,,AWM T"O G5],N ME?OD USES MULTIPLE

RECORD+S 7SAMPLES7 ( AN 9/RU;T ACR !

RANGE (! KEYBO>D2 ?US1 ! ACTUAL S.D (!

VOICE MAY 2 SLI<TLY DI6]5T F NOTE

6NOTE4

,NO?+ HAPP5S OR NO?+ SEEMS 6FUNC;N1 EV5

:5 PRESS+ A PANEL BUTTON4 ,= EXAMPLE1

PRESS+ ! ,,DEMO BUTTON DOES N />T !

,DEMO S;G1 OR PLAY+ ! KEYBO>D B#AAA

DOES N PRODUCE ANY S.D4

,"O (! ! DISK-RELAT$ 4PLAYS 7,,SAVE1

,,LOAD1 ,,DELETE1 OR ,,=MAT7 IS %[N4

,EXIT F ! 4PLAY 0PRESS+ ! ,,SAVE

BUTTON 7F ! ,,SAVE 4PLAY71 ! ,,LOAD

BUTTON 7F ! ,,LOAD 4PLAY71 OR !

,,UTIL;Y BUTTON 7F ! ,,DELETE OR

,,=MAT 4PLAYS74

,,DATA ,,BACKUP ,,& ,,9ITIALIZ,N

,EXCEPT =! DATA LI/$ 2L1 ALL ,,PSR-#CDJ

PANEL SETT+S >E RESET 6_! 9ITIAL SETT+S

:5"E ! P[] IS TURN$ ON4 ,! DATA LI/$ 2L

>E BACK$ UP--I4E4 RETA9$ 9 MEMORY--Z L;G

Z AN ;,,AC ADAPTOR IS 3NECT$ OR A SET (

BATT]IES IS 9/ALL$4

99 ,US] ,S;G ,DATA

99 ,METRONOME ,VOLUME

99 ,US] ,"O ,T\* ,SETT+ ,DATA

99 ,T\* ,ON/,(F

99 ,"O ,T\* ,SETT+ ,BANK ,NUMB]

99 ,T\* ,S5SITIV;Y

99 ,,EZ ,*ORD ,DATA

99 ,SPLIT ,PO9T C#AAA

99 ,,EZ ,*ORD ,BANK ,NUMB] ,DATA

99 ,A3OMPANI;T ,SPLIT ,PO9T

99 ,SM>T ,*ORD ,NUMB]

99 ,FOOTSWIT* ,ASSIGN ,FUNC;N

99 ,/YLE #AJA ,DATA

,,CAU;N3

99 ,ALL ,"O ,T\* ,SETT+ 7,US]7 & S;G

MEMORY DATA1 PLUS ! O!R SETT+S LI/$

ABV1 W 2 ERAS$ &/OR *ANG$ :5 ! DATA

9ITIALIZ,N PROC$URE IS C>RI$ \4

99 ,C>RY+ \ ! DATA 9ITIALIZ,N PROC$URE W

USU,Y RE/ORE NORMAL OP],N IF ! ,,PSR-

#CDJ FREEZES OR 2G9S 6ACT ]RATIC,Y =

ANY R1SON4

,DATA ,9ITIALIZ,N

,ALL DATA C 2 9ITIALIZ$ & RE/OR$ 6!

FACTORY PRESET 3DI;N 0TURN+ ON ! P[]

:ILE HOLD+ ! HI<E/ 7"RMO/7 :ITE KEY ON !

KEYBO>D4 8,,CL,'R ,BACKUP0 W APPE>

BRIEFLY ON ! 4PLAY4