#H

,,SETT+ ,,UP

,? SEC;N 3TA9S 9=M,N AB SETT+ UP YR

,PORTA,T"O = PLAY+4 ,MAKE SURE 6R1D ?

SEC;N C>E;LLY 2F US+ ! 9/RU;T4

,,P[] ,,REQUIRE;TS

,AL? ! ,,PSR-#CDJ W RUN EI F AN OP;NAL

;,,AC ADAPTOR OR BATT]IES1 ,YAMAHA

RECOMM5DS USE ( AN ;,,AC ADAPTOR :5"E

POSSI#4 ,AN ;,,AC ADAPTOR IS M

5VIRON;T,Y FRLY ?AN BATT]IES & DOES N

DEPLETE RES\RCES4

,,CAU;N

,N"E 9T]RUPT ! P[] SUPPLY 7E4G4 REMOVE !

BATT]IES OR UNPLUG ! ;,,AC ADAPTOR7 DUR+

ANY ,,PSR-#CDJ RECORD OP],N6 ,DO+ S C

RESULT 9 A LOSS ( DATA4

,US+ AN ;,,AC ,P[] ,ADAPTOR

,63NECT YR ,PORTA,T"O 6A WALL SOCKET1 Y

W NE$ ! OP;N,Y AVAILA# ,YAMAHA ,,PA-

#E;,B1 ,,PA-#E;,C OR ,,PA-#EA ,P[]

,ADAPTOR4 ,USE ( O!R ;,,AC A#H

ADAPTORS CD RESULT 9 DAMAGE 6! 9/RU;T1 S

2 SURE 6ASK =! "R K9D4 ,3NECT "O 5D (!

ADAPTOR 6! ,,DC ,,9 #AJ-AB;,V JACK ON !

RE> PANEL ( YR ,PORTA,T"O1 &! O!R 5D 6A

SUITA# ELECTRICAL \TLET4

,,W>N+

99 ,USE ,,ONLY A ,YAMAHA ,,PA-#E;,B1

,,PA-#E;,C OR ,,PA-#EA ;,,AC ,P[]

,ADAPTOR 7OR O!R ADAPTOR SPECIFIC,Y

RECOMM5D$ 0,YAMAHA7 6P[] YR 9/RU;T F

! ;,,AC MA9S4 ,! USE ( O!R ADAPTORS

MAY RESULT 9 IRREP>A# DAMAGE 6BO? !

ADAPTOR &! ,,PSR-#CDJ4

99 ,UNPLUG ! ;,,AC ,P[] ,ADAPTOR :5 N

US+ ! ,,PSR-#CDJ1 OR DUR+ ELECTRICAL

/ORMS4

,US+ ,BATT]IES

,9S]T+ ,BATT]IES

,TURN ! 9/RU;T UPSIDE-D[N & REMOVE !

BATT]Y -"P;T LID4 ,9S]T SIX #A.E-VOLT

SIZE 8;,D0 7,,SUM-#A1 ;,R-#BJ OR

EQUIVAL5T7 BATT]IES Z %[N 9 ! B#H

ILLU/R,N1 MAK+ SURE T ! POSITIVE &

NEGATIVE T]M9ALS >E PROP]LY ALIGN$1 &

REPLACE ! LID4

,',DIAGRAM3 ,9S]T+ ,BATT]IES

,:5 ! 9/RU;T IS UPSIDE-D[N1 ! BATT]Y

-"P;T IS LOCAT$ T[>D ! C5TRE BACK4 ,!

BATT]IES >E PLAC$ 96! -"P;T ) _!

POSITIVE T]M9ALS FAC+ LEFT4,'

,:5 ! ,BATT]IES ,RUN ,D[N

,:5 ! BATT]IES RUN L[ &! BATT]Y VOLTAGE

DROPS 2L A C]TA9 LEVEL1 ! ,PORTA,T"O MAY

N S.D OR FUNC;N PROP]LY4 ,Z SOON Z ?

HAPP5S1 REPLACE !M )A -PLETE SET ( SIX

NEW BATT]IES4

,,CAU;N

99 ,N"E MIX OLD & NEW BATT]IES OR DI6]5T

TYPES ( BATT]IES 7E4G41 ALKAL9E &

MANGANESE74

99 ,6PREV5T POSSI# DAMAGE F BATT]Y

L1KAGE1 REMOVE ! BATT]IES F ! 9/RU;T

IF X IS N 6BE US$ =A L;G "T4

,,TURN+ ,,ON ,,! ,,P[] C#H

,)! ;,,AC P[] ADAPTOR 3NECT$ OR )

BATT]IES 9/ALL$1 SIMPLY PRESS ! P[]

SWIT* UNTIL X LOCKS 9 ! ,,ON POSI;N4 ,:5

! 9/RU;T IS N 9 USE1 2 SURE 6TURN ! P[]

(F4 7,PRESS ! SWIT* AG S T X POPS UP47

,,CAU;N

,EV5 :5 ! SWIT* IS 9 ! 8,,/&BY0 POSI;N1

ELECTRIC;Y IS / FL[+ 6! 9/RU;T AT !

M9IMUM LEVEL4 ,:5 Y >E N US+ ! ,,PSR-

#CDJ =A L;G "T1 MAKE SURE Y UNPLUG !

;,,AC P[] ADAPTOR F ! WALL ;,,AC \TLET1

&/OR REMOVE ! BATT]IES F ! 9/RU;T4

--------------------------------------#I

,,A3ESSORY ,,JACKS

,US+ ,H1DPH"OS

,= PRIVATE PRACTIC+ & PLAY+ )\T 4TURB+

O!RS1 3NECT A SET ( /]EO H1DPH"OS 6! RE>

PANEL ,,PH"OS/,,\TPUT JACK4 ,S.D F !

BUILT-IN SP1K] SY/EM IS AUTOMATIC,Y CUT

(F :5 Y 9S]T A H1DPH"O PLUG 96? JACK4

,3NECT+ A ,KEYBO>D ,AMPLIFI] OR A#I

,/]EO ,SY/EM

,?\< ! ,PORTA,T"O IS EQUIPP$ )A BUILT-IN

SP1K] SY/EM1 Y C AL PLAY X "? AN EXT]NAL

AMPLIFI]/SP1K] SY/EM4 ,F/1 MAKE SURE !

,PORTA,T"O & ANY EXT]NAL DEVICES >E

TURN$ (F1 !N 3NECT "O 5D (A /]EO AUDIO

CA# 6! ,,L9E ,,9 OR ,,AUX ,,9 JACK7S7 (!

O!R DEVICE &! O!R 5D 6! RE> PANEL

,,PH"OS/,,\TPUT JACK ON ! ,PORTA,T"O4

,,CAU;N

,6PREV5T DAMAGE 6! SP1K]S1 SET ! VOLUME

(! EXT]NAL DEVICES AT ! M9IMUM SETT+ 2F

3NECT+ !M4 ,FAILURE 6OBS]VE ^! CAU;NS

MAY RESULT 9 ELECTRIC %OCK OR EQUIP;T

DAMAGE4 ,AL1 2 SURE 6SET ! VOLUMES ( ALL

DEVICES AT _! M9IMUM LEVELS & GRADU,Y

RAISE ! VOLUME 3TROLS :ILE PLAY+ !

9/RU;T 6SET ! DESIR$ LI/5+ LEVEL4

,US+ A ,FOOTSWIT*

,? F1TURE LETS Y USE AN OP;NAL FOOTSWIT*

7,YAMAHA ,,FC#D OR ,,FC#E7 6SU/A9 ! S.D

(! VOICES1 OR 3TROL A V>IETY ( O!R

FUNC;NS4 7,SEE PAGE #AJJ47 ,:5 ? B#I

IS US$ = SU/A91 ! FOOTSWIT* FUNC;NS !

SAME WAY Z A DAMP] P$AL ON AN AC\/IC

PIANO--PRESS & HOLD D[N ! FOOTSWIT* Z Y

PLAY ! KEYBO>D 6SU/A9 ! S.D4

,NOTE3

99 ,MAKE SURE T ! FOOTSWIT* PLUG IS

PROP]LY 3NECT$ 6! ,,FOOT ,,SWIT* JACK

2F TURN+ ON ! P[]4

99 ,D N PRESS ! FOOTSWIT* :ILE TURN+ !

P[] ON4 ,DO+ ? *ANGES ! RECOGNIZ$

POL>;Y (! FOOTSWIT*1 RESULT+ 9 REV]S$

FOOTSWIT* OP],N4

,US+ ,! ,,MIDI ,T]M9ALS

,! ,PORTA,T"O AL F1TURES ,,MIDI T]M9ALS1

ALL[+ Y 69T]FACE ! ,PORTA,T"O ) O!R

,,MIDI 9/RU;TS & DEVICES4 7,= M 9=M,N1

SEE PAGE #AJB47

,PACK+ ,LI/

99 ,,PSR-#CDJ

99 ,MUSIC ,/&

99 ,SAMPLE ,DISK

99 ,[N]'S MANUAL