# Jazz File List Installation Script

1 PRODUCT= Jazz Quick Start Installation
2 OEM=NO
3 CD=no
4 CDAUTOEXEC=
5 CDCONFIG=
6 DISKSPACE=1552694
7 DISKS=1
8 SOUNDSYSFILE=JAZZ.SYS
9 DEFAULTDIR=JAZZ
10 ARCHIVE=NO
11 SCSICONFIG=NO

PRESSF3=Press F3 to exit
ENTEREXIT=  ENTER=Continue  F3=Exit
ENTEREXITCANCEL=  Enter=Continue   F3=Exit   ESC=Escape
F3ISEXIT=F3=Exit
PCMCOM=pcm.com
PCMCOMARG=-l
PLAYEXE=play.exe
PLAYEXEARG=-TB16D4
PCMCOMSBC=-t%d,%d,%dl
PLAYEXESBC=-TB16D4
TESTWAV=test.wav
TESTDMAWAV=testdma.wav
TESTIRQWAV=testirq.wav
CHECKFILE=programs.lzh
SYSQUERY=qainfo -t204 -t205 -f scandos.txt

DISKNAME=Installation Diskette
+.
install.exe
filelist.txt
jazzinst.inf
jazz.sys
qainfo.exe
lharc.exe
programs.lzh

playfile.exe
pcm.com
play.exe
test.wav
testdma.wav
testirq.wav

(WINPKG) "prec.exe" "Pocket Recorder"
(WINPKG) "prec.hlp" "Pocket Recorder Help File"
(WINPKG) "jazzpmix.exe" "Pocket Mixer"
(WINPKG) "pkcd.exe" "Pocket CD Player"
(WINPKG) "pkcd.hlp" "Pocket CD Player Help File"

MFS0D=Install Software and Setup Hardware
MFS1D=Setup Hardware Only
MYN0D=YES
MYN1D=NO
MM0=Jazz I/O Port:
MM0D=220
MM1=Jazz IRQ:
MM1D=5
MM2=8 bit DMA:
MM2D=1
MM3=16 bit DMA:
MM3D=5
MM4=MPU-401 Enabled:
MM4D=
MM5=MPU-401 I/O Port:
MM5D=330
MM6=MPU-401 IRQ:
MM6D=2
MM7=Modify C: DOS System Files:
MM7D=YES
MM8=Modify    WIN System Files:
MM8D=YES
MM9=Complete Changes:
MM9D=Accept the configuration shown above

