[App]
;Application global information
AppName=MM CD16 Audio Setup
DefDir=C:\MMCD16
SpaceNeeded=2666539
DOSSpaceNeeded=1068099
GroupTitle=MM CD16 Audio Setup
GroupFile=MMCD16.GRP
WinDrvSect=MM16.DRV
CompanyName=AZI Labs.
Model=Clinton

[W95DrvInstall]
1=midi.inf
2=wave.inf
3=joystick.inf

SourcePath=.\win95

[midi.inf]
INFPath=.\win95
DrvDesc=MPU-401 Compatible
InstallSect=MPU401
Manufacturer=Microsoft
Provider=Microsoft
DelDrvKey=MPU-401

[wave.inf]
INFPath=.\win95
DrvDesc=AZT 1605 Audio Device
InstallSect=AZT1605_Device
Manufacturer=AZTECH
Provider=AZTECH
DelDrvKey=AZT 1605 Audio Device

[joystick.inf]
INFPath=.\win95
DrvDesc=Gameport Joystick
InstallSect=MSJSTICK
Manufacturer=Microsoft
Provider=Microsoft
DelDrvKey=Gameport

[Packages]
COMBINE1=1;enable aztech bundle
COMBINE2=0;disable voyetra bundle
NOEEPROM=0

[Languages]
;For foreign languages 
English =1, English.azt, English, English.txt
German  =1, German.azt,  German,  German.txt
French  =1, French.azt,  French,  French.txt
Dutch   =1, Dutch.azt,   Dutch,   Dutch.txt
Spanish =1, Spanish.azt, Spanish, Spanish.txt
Italian =1, Italian.azt, Italian, Italian.txt
password=aztech
default=english

[External Apps]
;AppsSetup=msetup.exe
;AppsTitle=Multi-Media Communicator Setup
;AppsDisk=4

[DOSEnv]
BLASTER=A220 I5 D1 T4
GALAXY=A220 I5 D1 P530 K10 T6

[Disks]
;List of diskettes needed to install the product and the name
;of each diskette.
1=Disk1: 

[DstDirs]
;lists of directories from root of destination drive/directory
;where destination files will be placed
1=.
2=DRIVERS
3=Windows
4=UTILITY
5=COMPRACK
6=SOUNDS
       
[Setup APP Files]
;These files will be copied to the root destination directory
1=setup.exe
2=setup.inf
3=setup.bmp
4=ENGLISH.AZT
;5=GERMAN.AZT   
;6=FRENCH.AZT 
;7=DUTCH.AZT
;8=SPANISH.AZT
;9=ITALIAN.AZT

[Files.english]
;identifier,disk,archive,subdirectory,shared,uncompressed size
1=1:README.COM,    1,  DOS, 16430
2=1:README.TXT,    1,  DOS, 4030
3=1:SETUP.INF,     1,  DOS, 5661
4=1:SETUP.EXE,     1,  DOS, 297840
5=1:DRIVERS.AZT,   2,  DOS, 106877
6=1:WINDOWS.AZT,   3,  WIN, 241411
7=1:UTILITY.AZT,   4,  DOS, 637261
8=2:COMPRACK.AZT,  5,  WIN, 1153910
9=2:SOUNDS.AZT,    6,  WIN, 203119


[DstDirs]
;lists of directories from root of destination drive/directory
;where destination files will be placed
1=.
2=DRIVERS
3=WINDOWS
4=UTILITY
5=COMPRACK
6=SOUNDS

[WinSys Files]                       
;identifier,subdirectory,file
1=3:mm16c.drv
2=3:mmopl3.drv
3=3:vsglx16.386
4=3:midimap.cfg
5=3:msacm.dll
6=3:msacm.drv
7=3:map_win.hlp
8=3:msadpcm.acm
9=3:msmixmgr.dll

[Windows Files]

[PM Info]                    
;identifier,subdirectory,file,description
1=4:winmixw.exe,    Mixer Control, 
2=5:clefstud.exe,   Clef Studio,
3=5:clefedit.exe,   Clef Edit,
4=5:clefole.exe,    Clef OLE,
5=1:setup.exe,      Audio Setup,

[WinSys.Drivers.Load]                    
;identifier,leftvalue,rightvalue
1=Wave,mm16c.drv
2=AUX,mm16c.drv
3=Midi,mm16c.drv
4=Mixer,mm16c.drv
5=Midi1,mmopl3.drv
6=Wavemapper,msacm.drv
7=Msacm.msadpcm.acm,msadpcm.acm

[WinSys.Drivers.Unload]         
;identifier,leftvalue,rightvalue
1=Wave,mm16c.drv
2=AUX,mm16c.drv
3=Midi,mm16c.drv
4=Mixer,mm16c.drv
5=Midi1,mmopl3.drv
6=Wavemapper,msacm.drv
7=Msacm.msadpcm.acm,msadpcm.acm

[WinSys.Boot]
;identifier,leftvalue,rightvalue,mode
1=drivers, msmixmgr.dll, APPEND

[WinSys.386Enh.Load]
;identifier,rightvalue(leftvalue is device=),mode
1=vsglx16.386, Install
2=vsglx16.386, Remove

[WinSys.386Enh.Unload]
;identifier,rightvalue(leftvalue is device=)
1=wsssb16.386
2=wsssbpro.386
3=vsndsys.386
4=vsgd.386
5=vsg16wss.386
6=vmm16wss.386
7=vsgb16ss.386
8=vmmb16ss.386
9=vvdmad.386

[WinControl]
;identifier,driver,description
1=mm16c.drv,16-bit Audio Driver
2=mmopl3.drv,FM driver
3=msacm.drv,Microsoft Sound Mapper V2.00
4=msacm.dll,Microsoft Sound Mapper DLL
5=map_win.hlp,Microsoft Sound Mapper Help File
6=msadpcm.acm,Microsoft ADPCM Audio Codec
7=msmixmgr.dll,Microsoft Mixer Manager

[WinAppIni]
1=CLEFSTUD.INI|CARD TYPE|TYPE|268
2=CLEFSTUD.INI|MODULE LIST|LIST|1 2 3 4
3=CLEFSTUD.INI|LAST PLAYLIST DIR|WAVE_DIR|$$$|SOUNDS
4=CLEFSTUD.INI|LAST PLAYLIST DIR|MIDI_DIR|$$$|SONGS
5=CLEFEDIT.INI|Defaults|StartDir|$$$|SOUNDS

[Hardware Settings]
;setting,combo box
;99 is disabled for CDROM DMA
;1:No CDROM, 2:LU005, 4:CR563, 5:CDU33A, 6:FX001, 7:CDA268
Base Port=220, 240
Wave Port=530, 604, E80, F40
MIDI Port=300, 330
Wave IRQ=7, 9, 10, 11
MIDI IRQ=2, 3, 5, 7
DMADAC=0, 1, 3
DMAADC=0, 1, 3
CDROM MODEL=2, 6, 4, 5, 7,8
CDROM IRQ=11, 12, 15
CDROM DMA=99, 3
Default Base Port=220
Default Wave Port=530
Default MIDI Port=330
Default Wave IRQ=10
Default MIDI IRQ=2
Default DMADAC=0
Default DMAADC=0
Default CDROM MODEL=7
Default CDROM IRQ=11
Default CDROM DMA=99

[W95DeletedHDID]
1=*PNP0802
2=*PNPB00D
3=*PNPB00E
4=*PNPB019
5=*PNPB007
6=*PNPB008
7=*PNPB000
8=*PNPB001
9=*PNPB002
10=*PNPB003
11=*CTL0001
12=*CTL0031
13=*CTL0021
14=*CTL8001
15=*PNPB004
16=*PNPB00B
17=*PNPB00D
18=*PNPB00E
19=*PNPB00F
20=*ESS6881
21=*ESS0100
22=*CPQA0D5
23=*ESS1481
24=*ESS4881
25=*ESS1681
26=*ESS0102
27=*CPQAE26
28=*AZT1605
29=*AZT2316
30=*PNPB006
31=*PNPB020
32=*PNPB02F
33=*AZT2316R
34=*AZT0000
35=*AZT0004
36=*AZT0005
37=*SB16.VXD
38=*SB16SND.DRV
39=*MSSBLST.VXD
40=*MSSBLST.DRV
41=*GAMEPORT JOYSTICK
42=*MPU-401 COMPATIBLE

[Autoexec]
;1=4|VOLSET|/V:14 /X:14 /F:14 /C:14 /L:14 /M:0 /R:M

[Config]
;1=DEVICE|2|EEPROM.SYS|/88BC0001

[End]
