PLEASE READ
-------------------------------------------------
By using the following Windows 3.1 Driver Library
(the "Software"), you are hereby agreeing to the
included license agreement.  Please review the
file LICENSE.TXT.


INSTALLING MEDIA VISION PRO AUDIOSPECTRUM DRIVERS 
-------------------------------------------------
Before you install the new Media Pro AudioSpectrum
drivers, you need to remove the old drivers. 


To remove the old Media Vision Pro AudioSpectrum
drivers: 

1  In the Main group, choose Control Panel.

2  In the Control Panel window, choose the Drivers
   icon. 

3  In the Installed Drivers list, select the driver
   you want to remove.
 
4  Choose the Remove button.

5  Choose the Yes button to confirm you want to
   remove this driver.

   Remove all Pro Audio Spectrum sound, MIDI, and
   mixer drivers.  Repeat the procedure for each
   driver you want to remove. DO NOT restart
   Windows until all Pro AudioSpectrum drivers have
   been removed.

6  Restart Windows, and then install the new Pro
   AudioSpectrum drivers.

NOTE:  When the dialog box appears asking if you wish
to install a "New" driver or use the "Current" driver,
select "New".  Windows prompts you to select the DMA
and interrupt.  Verify that the selections match your
board, and then choose the OK button.
