
                          Additional Information

                       MM CD16 Audio Setup Ver 1.01


   This file contains additional information and changes about the
   various software that was not available at printing time.

  
   Multimedia Sound Card Easy Start
   ================================
   There is an amendment to the above-mentioned documentation 
   (Page 5):

   "Your sound includes 3 built-in AT-Bus CD-ROM Drive interface 
   connectors. This allows you to connect either a Aztech, Mitsumi, 
   Mitsumi, Panasonic or Sony AT-Bus CD-ROM drive to your sound
   card." 


   Multimedia Sound Card User's Manual
   ===================================
   There is an amendment to the above-mentioned documentation
   (Page B-5).

   The CD-ROM Drive Options for the configuration program have been
   changed to the following:

   - Mitsumi LU005
   - Mitusmi FX001
   - Panasonic CR56x
   - Sony CDU33A
   - Aztech CDA268
   - No CD-ROM



   AT-BUS CD-ROM Drives Support
   ============================
   The sound card supports the following CD-ROM drives:

   Brand            Models
   -----            ------
   Panasonic    -   Model CR522/ 523/ 562 and 563
   Mitsumi      -   Model LU005S/ FX001D
   Sony         -   Model CDU31A/ 33A
   Aztech       -   Model CDA268-01A

   The bundled CD-ROM device drivers supports only the following drives:

   Driver           CD-ROM Model
   ------           ------------
   CR56X.SYS    -   Panasonic CR562 & CR563
   SGCDM.SYS    -   Mitsumi LU005S
   SGCD268.SYS  -   Aztech CDA268-01A


   Mitsumi CD-ROM Drivers
   ======================
   The original Mitsumi CD-ROM device driver does not support the CD-ROM
   Port Addresses (63xH & 65xH) used by your sound card. To overcome this
   problem, a patch program (CDPATCH.EXE) is bundled together with the 
   utility disk which can be found under the {...\DRIVERS} directory after 
   installing the sound card software.  This program will search and patch 
   the original Mitsumi CD-ROM drivers (i.e. MTMCDAE.SYS, MTMCDAS.SYS or 
   MTMCDE.SYS) in the {...\DRIVERS} directory automatically.

   The program will prompt the user before it proceed to modify the driver,
   and a message "... has been modified!" will be displayed upon successfully 
   modifying of the drivers.  If the driver is not the original version or
   it had been modified previously, the program will prompted "the file is 
   not modified!".

   Therefore, Please run this program immediately after the installation of 
   the original Mitsumi CD-ROM driver (via CONFIG.EXE utility and SETUP.EXE) 
   before rebooting your system to load the Mitsumi driver.


   Microsoft CD-ROM Extensions (MSCDEX.EXE)
   ========================================
   The above file is needed for operation of CD-ROM drives under the DOS
   environment. This file is only bundled with DOS version 6.x. Therefore, 
   if you are using DOS version 5, please contact your local Microsoft's
   dealers for a copy of MSCDEX.EXE (for DOS version 5 usage).


   Installation on Win3.1x Platform
   ================================
   On Windows 3.1x Operating System, choose 'Run' from the 'File' menu. Insert
   the Audio Installation Disk#1 into Drive A: (or Drive B:) and change the path
   to A:\setup (or B:\setup). For more details, you can refer to the Easy Start 
   Manual.


   Installation on Windows 95 Platform
   ===================================
   Start up Windows 95 Operating System. Choose 'Run' from the 'Start' menu and
   insert the Audio Installation Disk#1 into Drive A: (or Drive B:) and change
   the path to 'A:\setup.exe' (or B:\setup.exe) and click OK to install the
   audio drivers as well as the application software.


   Upgrading from Win3.x to Win95 platform
   =======================================
   If you have set up your audio card on a Win3.x platform and want to upgrade
   to Windows 95, remember to remove the audio drivers by doing a deinstallation
   first. For more details, you can refer to the Appendix section in the User's
   Manual.
   


        ***********************************************************
        *  In case you encounter any problem with our products,   *
        *  please quote the following model(s) when calling our   *
        *  Technical Support :                                    *
        *                                                         *
        *                     P16(CD)-3/-P/-PA/-PAII Sound Card   *
        *                                                         *
        *********************************************************** 



                        -------  The End  ---------

