//--------------------------------------------------------------------
//
// INSTALL on-line Help Text File 
//
// Help Customization Guidelines:
//
// 0) Comment lines start with leading '//'.
// 1) Help Message Text starts with #MESSAGE statement
// 2) Never change the number after the #MESSAGE statement. That is
//    the search Message ID for the INSTALL program.
// 3) LINES statement defines how many (lines) x (characters) allowed.
//    Never exceed this limits when you type the text for the message.
// 4) TITLE statement defines the sub-Title of this message.
//    (allow to modify for your customization)
// 5) Text area starts and ends with a '$'.
//    (allow to modify for your customization)  
// 6) the INSTALL program is not going to format your 
//    text. It just show whatever text you typed here 
//    line by line. So you have to do the formatting for
//    better effect and please use SPACEs but not TABs.   
//    (you don't need to enter trailing SPACE lines. If there is space
//     left at the bottom of a HELP message, white space is the default.)
// 7) Anyway, give a try and see how it goes.
//
// 9) Format Overview (example)
//
//    #MESSAGE = 1                         // starts Help message 1
//    TITLE="Selcet CD-ROM Type"        // sub-title of this message
//    LINES=9x50                        // allowed text area: 
//                                      // 9 lines x 50 characters
//    $	                                // starts text area
//    TEXT LINEs
//    TEXT """"	                        // help text
//    " " "
//    $                                 // end of text area
//-----------------------------------------------------------------    

//
// INSTALL Help Text: Message by Message
//

#MESSAGE = 1
TITLE="W E L C O M E"
LINES=9x48
$
INSTALL is a complete installation and
test program for 82C931 sound device.
A mouse is recommended. If you do not
have a mouse, use the following keys:
  [TAB]       to move to option
  [ENTER]     to execute option
  []        to select option 
  [F3]        to exit the installation
  [ALT+Key]   to activate a button 
$
 
#MESSAGE = 20
TITLE="TEST & CONFIGURATION OPTIONS"
LINES=6x52
$
The Test and Configuration program will allow you:
- Configure and Test your Sound Card
- Change CD-ROM settings and update system files
- Perform 8 bit, 16 bit and FM Music Sound Tests
- Change volume settings
- View information file README.TXT
$

#MESSAGE = 5
TITLE="CD-ROM SELECTION"
LINES=4x44
$
MAD16 Pro sound card can be used as a CD-ROM 
interface board.  Select your CD-ROM drive
type or select [None] if you do not want to
connect the CD-ROM drive to the sound card.
$


#MESSAGE = 7
TITLE="CD-ROM HARDWARE CONFIGURATION"
LINES=5x48
$
Select [OK] if you accept the settings for your
CD-ROM. 
 
Select [DEFAULTS] if you want to set the CD-ROM
to the default settings.
$


#MESSAGE = 13
TITLE="Select MSCDEX.EXE For CD-ROM"
LINES=7x44
$
The following is MSCDEX(s) on your system. Please
select one compatible with your DOS version.

* For DOS/Windows 3.1, use the one which came 
  with DOS.
* For Windows 95/DOS, use the one which came 
  with Windows 95.
$

#MESSAGE = 14
TITLE="No MSCDEX.EXE in your system"
LINES=10x50
$
To use your CD-ROM Drive, you need the program
MSCDEX.EXE from Microsoft.  INSTALL has scanned 
your hard disk(s) and did not find one. Besides, 
your DOS version is very old. We don't have a 
MSCDEX version good for you. INSTALL inserted a 
MSCDEX line with leading 'REM' to the AUTOEXEC.BAT
anyway. If you locate a MSCDEX file later, please 
copy it to the MAD16 Pro directory and remove the
REMark of MSCDEX line in AUTOEXEC.BAT .
$

#MESSAGE = 15
TITLE="SYSTEM FILES UPDATE"
LINES=7x48
$
INSTALLER is going to update your system files
CONFIG.SYS and AUTOEXEC.BAT.

Select [OK] if you want INSTALLER to make the
changes NOW or select [BACKUP ONLY] if you
want INSTALLER only to save the changes to
the backup files CONFIG.MAD and AUTOEXEC.MAD.
$

#MESSAGE = 19
TITLE="Not Enough Conventional Memory Detected"
LINES=10x56
$
Your system has LESS THAN 500 KBytes of recommended 
conventional memory. To run DOS games, you need at 
least the recommended size above. It is also
recommended that this amount of memory be available
in order to successfully run this program. You can 
increase your memory either by running a memory maker 
program that comes with your operating system, or 
remove any memory resident programs that resides in 
the system memory. Do you wish to EXIT this program 
and increase your system memory now?
$

#MESSAGE = 22
TITLE="W E L C O M E"
LINES=9x42
$
SNDINIT is the testing and configuration
program for 82C931 sound device. A mouse
is recommended. If without a mouse, you
may use the following keys:
  [TAB]       to move to option
  [ENTER]     to execute option
  []        to select option 
  [F3]        to exit the program
  [ALT+Key]   to activate a button 
$

#MESSAGE = 23
TITLE="CD-ROM DRIVER INSTALLATION" 
LINES=6x48
$
Installer does not have the CD-ROM driver for
your CD-ROM. Installer will only update the 
the CD-ROM settings of the sound card in 
CONFIG.SYS. Please run the installation program
from your CD-ROM manufacturer to install the 
CD-ROM driver and MSCDEX program.
$

#MESSAGE = 24
TITLE="REBOOT SYSTEM" 
LINES=5x49
$
Your CONFIG.SYS has been updated according to 
the new settings for your CD-ROM. You must REBOOT
your computer in order for the new settings to 
take effect. Select [OK] to REBOOT your computer.
Select [EXIT] to continue without reboot.
$

#MESSAGE = 25
TITLE="REBOOT SYSTEM"
LINES=4x46
$
Your BLASTER Environment Variable is updated
in your AUTOEXEC.BAT file. Some DOS games may
reference this variable for initialization
purposes. Do you wish to REBOOT your computer?
$

#MESSAGE = 26
TITLE="Error!"
LINES=2x48
$
Hardware Error Detected! Please reconfigure your
Sound Card's I/O Port, IRQ, or DMA settings.
$

#MESSAGE = 27
TITLE="Error!"
LINES=4x45
$
You have selected the same I/O Port setting
between your Audio, CD-ROM, or MPU-401
device. This will cause conflict on your
system. Please reselect a different I/O Port.
$

#MESSAGE = 28
TITLE="Error!"
LINES=4x47
$
You have selected the same IRQ settings between
your Audio, CD-ROM, Modem, or MPU-401 device.
This will cause conflict on your system. Please
reselect a different IRQ setting.
$

#MESSAGE = 29
TITLE="Error!"
LINES=4x47
$
You have selected the same DMA settings between
your Audio, and CD-ROM device. This will cause
conflict on your system. Please reselect a
different DMA setting.
$

#MESSAGE = 30
TITLE="Warning!"
LINES=3x48
$
You have selected Windows Sound System using IRQ
5.  Some DOS games that support Windows Sound
System may not work with this option.  
$

#MESSAGE = 35
TITLE="AUDIO DEVICE NOT ENABLED"
LINES=6x48
$
There is no proper audio resources assigned for
your sound card. To play DOS games or to run 
Audio applications, resources must be assigned 
to the audio device. Please check the audio 
configuration to see if there is any conflict 
with other devices on your system.
$

#MESSAGE = 36
TITLE=""
LINES=2x15
$
Disabled
I/O:2e8 IRQ:3
$

#MESSAGE = 37
TITLE=""
LINES=4x20
$
Disabled
I/O:36e,168 IRQ:10
I/O:376,170 IRQ:15
I/O:3ee,1e8 IRQ:11
$

#MESSAGE = 38
TITLE="16-BIT DMA"
LINES=2x48
$
Some games use Sound Blaster commands may
not work for the current DMA settings. 
$

#MESSAGE = 41
TITLE="~C~ontinue"
LINES=1x5
$
41
$

#MESSAGE = 42
TITLE="System Memory Detected:"
LINES=1x5
$
42
$

#MESSAGE = 43
TITLE="Recommended Memory:      1024 KB"
LINES=1x5
$
43
$

#MESSAGE = 44
TITLE="~S~tart Installation"
LINES=1x5
$
44
$

#MESSAGE = 45
TITLE="~C~onfigure & Test Sound Card"
LINES=1x5
$
45
$
 
#MESSAGE = 46
TITLE="~V~iew README.TXT"
LINES=1x5
$
46
$

#MESSAGE = 47
TITLE="~E~xit"
LINES=1x5
$
47
$
     
#MESSAGE = 49
TITLE="~O~K"
LINES=1x5
$
49
$

#MESSAGE = 50
TITLE="  Required disk space:"
LINES=1x5
$
50
$

#MESSAGE = 51
TITLE="  Available on drive"
LINES=1x5
$
51
$
	   
#MESSAGE = 54
TITLE="Enter your Windows directory"
LINES=1x5
$
54
$

#MESSAGE = 55
TITLE="~C~ANCEL"
LINES=1x5
$
55
$

#MESSAGE = 56
TITLE="~N~ONE"
LINES=1x5
$
56
$

#MESSAGE = 59
TITLE="N/A"
LINES=1x5
$
59
$

#MESSAGE = 60
TITLE="~C~HANGE"
LINES=1x5
$
60
$

#MESSAGE = 70
TITLE="Select your CD-ROM drive type"
LINES=1x5
$
70
$

#MESSAGE = 71
TITLE="CD-ROM Drive List:"
LINES=1x5
$
71
$

#MESSAGE = 72
TITLE="Your CD Drive:"
LINES=1x5
$
72
$

#MESSAGE = 73
TITLE="Disabled"
LINES=1x5
$
73
$

#MESSAGE = 74
TITLE="Enabled"
LINES=1x5
$
74
$

#MESSAGE = 75
TITLE="Searching for MSCDEX.EXE(s) on your system."
LINES=1x5
$
75
$

#MESSAGE = 76
TITLE="Please wait..."
LINES=1x5
$
76
$

#MESSAGE = 77
TITLE="CONFIGURATION"
LINES=5x25
$
~S~OUND TEST
~H~ELP
~D~EFAULT
~A~CCEPT
MI~X~ER
$

#MESSAGE = 78
TITLE=""
LINES=7x35
$
Sound Device Settings Selection
 Current Mode:
Sound Blaster Pro      IO Port:
Windows Sound System   IO Port:
     IRQ:
Play DMA:
$

#MESSAGE = 79
TITLE=""
LINES=6x25
$
Additional Options
Joystick:
MPU401 Interface
Interface:
  IO Port:
      IRQ:
$

#MESSAGE = 80
TITLE=""
LINES=5x25
$
Sound Card CD-ROM Interface
  Modem:
Record DMA:
$

#MESSAGE = 81
TITLE=""
LINES=5x25
$
Sound Blaster Pro
Windows Sound System
ON
OFF
$


#MESSAGE = 90
TITLE="Select a Sound Test Option"
LINES=4x50
$
Performing Sound Test. If you do not hear any
sound, please check that your speakers are
connected properly; or reconfigure your
hardware settings and select Sound Test again.
$

#MESSAGE = 91
TITLE=""
LINES=3x25
$
8-bit Sound Test
16-bit Sound Test
FM Synthesis Test
$

#MESSAGE = 92
TITLE="Sound Test Failed. Please reconfigure your"
LINES=1x5
$
92
$

#MESSAGE = 93
TITLE="Sound Blaster options and select "
LINES=1x5
$
93
$

#MESSAGE = 94
TITLE="Windows Sound System options and select "
LINES=1x5
$
94
$

#MESSAGE = 95
TITLE="Error! Not enough memory to play wave file."
LINES=2x50
$
Error! Sound Test has detected a wave file 
format which it cannot play.
$

#MESSAGE = 96
TITLE=""
LINES=2x50
$
Error! The wave file for Sound Test could not
be found. Please verify its location.
$

#MESSAGE = 97
TITLE="~D~ONE"
LINES=3x25
$
8-bit ~S~ound Test
16-bit Sound ~T~est
~F~M Synthesis Test
$

#MESSAGE = 98
TITLE="MSCDEX File List:"
LINES=2x25
$
MSCDEX File List:
Your Selection:
$

#MESSAGE = 99
TITLE="~B~ACKUP ONLY"
LINES=1x5
$
99
$

#MESSAGE = 100
TITLE="~R~EBOOT"
LINES=1x5
$
100
$

#MESSAGE = 101
TITLE="~E~XIT"
LINES=1x5
$
101
$

#MESSAGE = 102
TITLE="Error! Not enough memory to run program."
LINES=7x65
$
Warning! This program has detected that you do not
have the recommended 490 KBytes of conventional
memory available to run this program. Please remove
any memory resident programs that reside in your
system and run this program again. Consult your
operating system manual for details on increasing
the conventional memory in your system.
$

#MESSAGE = 103
TITLE=""
LINES=4x65
$
Warning! This program cannot be executed under a
Windows MS-DOS Prompt Session. Please type EXIT
to return to Windows and quit your Windows session
before running this program again.
$

#MESSAGE = 104
TITLE="Online Help and Information"
LINES=4x45
$
   [TAB]     to move to option
   [Enter]   to execute to option
   [F3]      to exit the program
   [ALT+Key] to activate a button
$
   
#MESSAGE = 105
TITLE=""
LINES=6x45
$
   No OPTi audio chips found
   OPTi 82C%d audio chips found
   Unknown chips found
   No CODEC found
   CODEC %d found
   Unknown CODEC found
$

#MESSAGE = 106
TITLE=""
LINES=3x50
$
  Warning! GPOUT of MIXER.CFG is available
  for 929 chip only. Please correct the 
  settings in MIXER.CFG. Thank you.
$

#MESSAGE = 107
TITLE=""
LINES=11x35
$
Master
Mute:
On
Off
Recording:
Source:
Gain:
Additional Control:
D~E~FAULT
~D~ONE
~I~NFOMATION
Mono Gain
$

#MESSAGE = 108
TITLE=""
LINES=3x45
$
Could not find list file for DISK 1.
Installer Could not find DISK 1.
Installer error: Out of memory.
$

#MESSAGE = 109
TITLE=""
LINES=4x60
$
Sound Card Initialization Error!
Your SET %s environment variable is not defined.
Please verify that the above variable is defined
in your AUTOEXEC.BAT file.
$

#MESSAGE = 110
TITLE=""
LINES=6x50
$
Initialization Error!
The Audio Configuration file %s.cfg could
not be found at the
following location:  %s
The CDROM Configuration file CDROM.CFG 
could not be found 
$

#MESSAGE = 111
TITLE=""
LINES=1x50
$
Error! Not enough memory to run program.
$

#MESSAGE = 112
TITLE="     Initializing sound card in "
LINES=1x5
$
112
$

#MESSAGE = 113
TITLE="Sound Blaster Pro Mode..."
LINES=1x5
$
113
$

#MESSAGE = 114
TITLE="Windows Sound System Mode..."
LINES=1x5
$
114
$

#MESSAGE = 115
TITLE="                Port Address: "
LINES=1x5
$
115
$

#MESSAGE = 116
TITLE="                 IRQ Channel: "
LINES=1x5
$
116
$

#MESSAGE = 117
TITLE="                 DMA Channel: "
LINES=1x5
$
117
$

#MESSAGE = 118
TITLE="        DMA Playback Channel: "
LINES=1x5
$
118
$

#MESSAGE = 119
TITLE="         DMA Capture Channel: "
LINES=1x5
$
119
$

#MESSAGE = 120
TITLE="            CD-ROM Interface: "
LINES=1x5
$
120
$

#MESSAGE = 121
TITLE="         CD-ROM Port Address: "
LINES=1x5
$
121
$

#MESSAGE = 122
TITLE="          CD-ROM IRQ Channel: "
LINES=1x5
$
122
$

#MESSAGE = 123
TITLE="          CD-ROM DRQ Channel: "
LINES=1x5
$
123
$

#MESSAGE = 124
TITLE="            Game Port Access: "
LINES=1x5
$
124
$

#MESSAGE = 125
TITLE="         Input Source Select: "
LINES=1x5
$
125
$

#MESSAGE = 126
TITLE="           MPU-401 Interface: "
LINES=1x5
$
126
$

#MESSAGE = 127
TITLE="        MPU-401 Port Address: "
LINES=1x5
$
127
$

#MESSAGE = 128
TITLE="         MPU-401 IRQ channel: "
LINES=1x5
$
128
$

#MESSAGE = 129
TITLE=""
LINES=5x15
$
CD
MIDI
WAVE
LINE
MIC
$
