Note: This Apollo2 driver is setup for the following configuration:

- Apollo2 Speech Synthesizer
- COM1
- 9600 Baud
- U.S. English Speech in ROM socket #1
- Spanish in ROM socket #2, with no other languages loaded in other sockets
- English is the language for the menus and the primary reading voice
- Spanish is the second reading voice

You should have the English version of An Open Book with U.S. English and
Spanish Recognition disks.

Note: There is a complete multi-language (U.S.English, French, German, Italian)
example of a APOLLO2.INI file. It can be found in the DOLPHIN directory,
the file name is APOLLO2.TXT. This file can be modified to match the 
languages that you have in your Apollo2 synthesizer and then renamed 
APOLLO2.INI, copied to the A2E&S directory and used as a "other" driver
during install.

Note: All .INI files for speech synthesizers from Dolphin Oceanic are named 
APOLLO2.INI.
