Stereo Volume Control

The following stereo volume commands are supported. DD1 or DD2 must be in the range of 0 to 99.

SYNTAX: | [:volume XX DD1 DD2]
ABBREVIATION: | [:volu XX DD1 DD2]]
ALTERNATE COMMAND: | [:volume XX DD]

OPTIONS: | lset | Sets the left channel to the desired level
| lup | Increases the left channel by the desired amount
| ldown | Decreases the left channel by the desired amount
| rset | Sets the right channel to the desired level
| rup | Increases the right channel by the desired amount
| rdown | Decreases the right channel by the desired amount
| sset | Sets the left channel to the DD1 amount and the right channel to the DD2 amount

PARAMETERS: | Volume amount(s)
DEFAULT: | none
EXAMPLES: | [:volume sset 80 60]