BrailleNote and VoiceNote BT GPS V4.0 Command summary

Description and BT command

Where am I commands: SPACE with H, W

Nearest intersection if you are not moving, next intersection if you are moving: X or dots 4-5-6

Detailed description of intersection: SPACE with X or dots 4-6

Nearest street address: A

Current city: C

Detailed description of your current location: SPACE with C

Heading compass and degrees: H or dot 5

Latitude and longitude: Y

Altitude: Z

Which mode am I in? GPS or Virtual: SPACE with I

GPS commands: SPACE with H, G

Speed: S

Approximate GPS distance, accuracy, and number of satellites: G or SPACE with dot 5

Quality and detailed GPS accuracy: Q

Switch to GPS mode: V

Distance between virtual and GPS positions: I

Greenwich mean time: U

Set Braillenote time to GPS time: SPACE with U

Set GPS receiver: O, G

Reconnect to Bluetooth GPS receiver: BACKSPACE with R 

Toggle Pause/Resume GPS Replay: BACKSPACE with Q

Start/Stop Recording GPS Replay: SPACE with Q

Virtual commands: SPACE with H, V

Switch to Virtual mode: V

Set virtual position by address: SPACE with S

Set virtual position to POI or Waypoint: SPACE with V

Set virtual position to GPS position: SPACE with G

Set virtual position by Latitude and Longitude: SPACE with Y

Distance between virtual and GPS positions: I

Move forward one intersection: dots 2-3-5-6

Turn to next street on left: dots 2-3

Turn to next street on right: dots 5-6

Move backward one intersection: SPACE with dots 2-3-5-6

Destination commands: SPACE with H, D

Heading and distance to destination: D or ENTER with dots 5-6

Set destination by address: SPACE with S

Set destination to POI or Waypoint: SPACE with D or SPACE with dot 6

Set destination by Latitude and Longitude: SPACE with Y

Points of interest commands: SPACE with H, P

Find nearest points in all categories: F or dot 4

Advance Find POI in all or individual categories between a beginning and ending distance: SPACE with F

Announce current POI: P or dot 3

Announce detailed description of current POI: SPACE with P

Create a User POI at GPS or Virtual Position: SPACE with dot 3

Create User POI by address: SPACE with S

Create POI from Latitude and Longitude: SPACE with Y

Edit user points of interest: E, P

Move to next POI: SPACE with dot 4

Move to previous POI: SPACE with dot 1

Nearest POI: SPACE with dots 1-2-3

Furthest POI: SPACE with dots 4-5-6

Jump forward 10 POIs: SPACE with dots 5-6

Jump back 10 POIs: SPACE with dots 2-3

Route commands: R

Route Announcement commands List: R, A

Current Waypoint: K or dot 2

Nearest Waypoint: N

Next turn or road transition: T or BACKSPACE with dots 2-3

Route distance and ETA from current position to Explore Waypoint: R, A, G

Total route distance: R, A, D

Announce Route distance from beginning of route to current position: R, A, B

Announce Route distance and ETA from current position to end of the route: R, A, E

Route management commands List: R, M

Set current Waypoint nearest GPS position: SPACE with N

Edit route: E, R

Add current POI as a Waypoint: R, M, P

Add current GPS or virtual position as Waypoint: SPACE with K or SPACE with dot 2

Route Settings commands List: R, T

Auto increment Waypoint on/off GPS mode: R, T, A

Force sequential route following GPS mode: R, T, F

Toggle between route turns and waypoints GPS mode: R, T, M

Waypoint numbering on/off GPS mode: R, T, G

Waypoint numbering on/off Virtual mode: R, T, V

Auto Recalculate Route: R, T, R

Create pedestrian route: R, P

Create vehicle route: R, V

Create manual route: R, O

Open route: R, O

Save route: R, S

Close route: R, C

Explore Route next Waypoint: dots 2-3-5-6

Explore Route previous Waypoint: SPACE with dots 2-3-5-6

Explore Route next Turn: dots 3-6

Explore Route previous Turn: SPACE with dots 3-6

Recalculate route: BACKSPACE with dot 3

Reverse route: R, R

Percent of route completed and ETA: dots 1-4-6

Route information: R, I

LookAround commands: SPACE with M

LookAround on/off Toggle: SPACE with M, L

Commercial POIs: on or off: if on which category-sub category: SPACE with M, P

Intersections: on or off: SPACE with M, X

User POIs: on or off: SPACE with M, U

Commercial POI Categories: SPACE with M, C

Multiple repeat commands: M

Turn off all Multiple Repeat commands: M, M

Multiple Repeat Delay: M, R

Trigger Multiple Repeat Announcements Manually: BACKSPACE with dot 1

Intersections: M, X

Detailed Intersections: M, N

Heading: M, H

Destination: M, D

Virtual: M, V

Route Next Waypoint: M, K

Route Next Turn: M, T

Route ETA: M, E

Speed: M, S

GPS Status: M, G

City: M, C

Address: M, A

Current POI: M, P

Altitude: M, Z

Latitude and Longitude: M, Y

Miscellaneous commands: SPACE with H, C

Pedometer GPS accumulated distances: B

Pedometer Virtual accumulated distances: B

Reset GPS pedometer: SPACE with B

Reset Virtual pedometer: SPACE with B

Lock or unlock the keyboard: ENTER with L

Spell name: SPACE with dots 2-5

Redo last command: SPACEBAR

Repeat last announcement: SPACE with R or L

Interrupt speech: BACKSPACE with ENTER

Append last spoken item to clipboard: BACKSPACE with K

Option commands: O

Map and POI Folder: O, M

Heading Mode: O, H

Street Name Short/Long: O, N

Units: O, U

Arrival Distance: O, D

Near Threshold: O, T

GPS Receiver Selection: O, G

Braille Display Delay: O, B

SPACE BAR Activates Last Command: O, C

Sounds Menu: O, S

Turn On/Off all Sounds: O, S, S

Play Nearest Intersection: O, S, X

Play Background operation: O, S, B

Play Destination Arrival: O, S, D

Play Virtual Arrival: O, S, A

Play Route Waypoint Turn Now: O, S, T

Play Route Turn Around: O, S, E

Play Route Continue Straight: O, S, C

Play Route Off Route: O, S, O

Play Route Recalculating Pedestrian: O, S, P

Play Route Recalculating Vehicle: O, S, V

Sendero Documentation: SPACE with H, S

Quick Reference Guide: SPACE with H, s, Q

Sendero GPS Manual: SPACE with H, S, S

Exit GPS: SPACE with E