BrailleNote and VoiceNote QT GPS V4.0 Command summary

Description and QT command


Where am I commands: HELP then W

Nearest intersection if you are not moving, next intersection if you are moving: X

Detailed description of intersection: READ with X

Nearest street address: A

Current city: C

Detailed description of your current location: READ with C

Heading compass and degrees: H

Latitude and longitude: Y

Altitude: Z

Which mode am I in? GPS or Virtual: READ with I

GPS commands: HELP then G

Speed: S

Approximate GPS distance, accuracy, and number of satellites: G

Quality and detailed GPS accuracy: Q

Switch to GPS mode: V

Distance between virtual and GPS positions: I

Greenwich mean time: U

Set Braillenote time to GPS time: READ with U

Change GPS receiver: O, G

Reconnect to Bluetooth GPS receiver: CONTROL with R

Toggle Pause/Resume GPS Replay: CONTROL with Q

Start/Stop Recording GPS Replay: READ with Q

Virtual commands: HELP then V

Switch to Virtual mode: V

Set virtual position by address: READ with S

Set virtual position to POI or Waypoint: READ with V

Set virtual position to GPS position: READ with G

Set virtual position by Latitude and Longitude: READ with Y

Distance between virtual and GPS positions: I

Move forward one intersection: CONTROL Up Arrow

Turn to next street on left: CONTROL Left Arrow

Turn to next street on right: CONTROL Right Arrow

Move backward one intersection: CONTROL Down Arrow

Destination commands: HELP then D

Heading and distance to destination: D

Set destination by address: READ with S

Set destination to POI or Waypoint: READ with D

Set destination by Latitude and Longitude: READ with Y

Points of interest commands: HELP then P

Find nearest points in all categories: F

Advance Find POI in all or individual categories between a beginning and ending distance: READ with F

Announce current POI: P

Announce detailed description of current POI: READ with P

Create a User POI at GPS or Virtual Position: READ with R

Create POI by address: READ with S

Create POI from Latitude and Longitude: READ with Y

Edit user points of interest: E, P

Move to next POI: down Arrow

move to previous POI: Up Arrow

Nearest POI: READ with T

Furthest POI: READ with B

Jump forward 10 POIs: Right Arrow

Jump back 10 POIs: Left Arrow

Route commands: R

Route Announcement commands List: R, A

Current Waypoint: K

Nearest Waypoint: N

Next turn or road transition: T

Route distance and ETA from current position to Explore Waypoint: R, A, G

Total route distance: R, A, D

Announce Route distance from beginning of route to current position: R, A, B

Announce Route distance and ETA from current position to end of the route: R, A, E

Route management commands List: R, M

Set current Waypoint nearest GPS position: READ with N

Edit route: E, R

Add current POI as a Waypoint: R, M, P

Add current GPS or virtual position as Waypoint: READ with K

Route Settings commands List: R, T

Auto increment Waypoint on/off GPS mode: R, T, A

Force sequential route following GPS mode: R, T, F

Toggle between route turns and waypoints GPS mode: R, T, M

Waypoint numbering on/off GPS mode: R, T, G

Waypoint numbering on/off Virtual mode: R, T, V

Auto Recalculate Route: R, T ,R

Top Level Route Commands: no sub menu for these commands

Create pedestrian route: R, P

Create vehicle route: R, V

Create manual route: R, O

Open route: R, O

Save route: R, S

Close route: R, C

Explore Route next Waypoint: READ with UP ARROW

Explore Route previous Waypoint: READ with DOWN ARROW

Explore Route next Turn: READ with RIGHT ARROW

Explore Route previous Turn: READ with LEFT ARROW

Recalculate route: BACKSLASH or SLASH

Reverse route: R, R

Percent of route completed and ETA: %

Route information: R, I

LookAround commands: READ with M

LookAround on/off Toggle: READ with M, L

Commercial POIs: on or off: if on which category-sub category: READ with M, P

Intersections: on or off: READ with M, X

User POIs: on or off: READ with M, U

Commercial POI Categories: READ with M, C

Multiple repeat commands: M

Turn off all Multiple Repeat commands: M, M

Multiple Repeat Delay: M, R

Trigger Multiple Repeat Announcements Manually: CONTROL with S

Intersections: M, X

Detailed Intersections: M, N

Heading: M, H

Destination: M, D

Virtual: M, V

Route Next Waypoint: M, K

Route Next Turn: M, T

Route ETA: M, E

Speed: M, S

GPS Status: M, G

City: M, C

Address: M, A

Current POI: M, P

Altitude: M, Z

Latitude and Longitude: M, Y

Miscellaneous commands: HELP then C

Pedometer GPS accumulated distances: B

Pedometer Virtual accumulated distances: B

Reset GPS pedometer: CONTROL with B

Reset Virtual pedometer: CONTROL with B

Lock or unlock the keyboard: CONTROL with L

Spell name: CONTROL with K

Redo last command: SPACEBAR

Repeat last announcement: REPEAT key

Interrupt speech: READ with SPACE

Append last spoken item to clipboard: CONTROL with C

Option commands: O

Map and POI Directory: O, M

Heading Mode: O, H

Street Name Detailed: O, N

Units: O, U

Arrival Distance: O, D

Near Threshold: O, T

GPS Receiver Selection: O, G

Braille Display Delay: O, B

SPACEBAR Activates Last Command: O, C

Sounds Menu: O, S

Turn On/Off all Sounds: O, S, S

Play Nearest Intersection: O, S, X

Play Background operation: O, S, B

Play Destination Arrival: O, S, D

Play Virtual Arrival: O, S, A

Play Route Waypoint Turn Now: O, S, T

Play Route Turn Around: O, S, E

Play Route Continue Straight: O, S, C

Play Route Warning Off Route: O, S, O

Play Route Recalculating Pedestrian: O, S, P

Play Route Recalculating Vehicle: O, S, V

Sendero Documentation: HELP then S

Quick Reference Guide: HELP then S, Q

Sendero GPS Manual: HELP then S, S

Exit GPS: ESCAPE